Abstract Test Suite for UNI 3.1 Signalling for the Network Side af-test-0090.000

ATM Forum Technical Committee

5. Abbreviations

AALP ATM Adaptation Layer Parameters ATD ATM Traffic Descriptor ATM Asynchronous T ransfer Mode ATS Abstract T est Suite BBC Broadband Bearer Capability BHL Broadband High Layer information BLL Broadband Low Layer information BRI Broadband Repeat Indicator BSC Broadband Sending Complete CA Cause CALL PROC CALL PROCeeding message CDN Called party Number CDS Called party Sub-address CGN Calling party Number CGS Calling party Sub-address CI Connection Identifier CONN CONNect message CONN ACK CONNect ACKnowledge message CR Call Reference CS Call State FIFO First In/First Out IE Information Element ISO/IEC International Organization for Standardization/International Electrotechnical Commission IUT Implementation Under T est MT Message Type PCO Point of Control and Observation PDU Protocol Data Unit PHY Physical Layer PICS Protocol Implementation Conformance Statement PIXIT Protocol Implementation eXtra Information for T esting QOS Quality Of Service

Page 5-1

Abstract Test Suite for UNI 3.1 Signalling for the Network Side af-test-0090.000

ATM Forum Technical Committee

RELEASE RELEASE message RELEASE COMP RELEASE COMPlete message RESTART RESTART message RESTART ACK RESTART ACKnowledge message RI Restart Indication SETUP SETUP message TNS Transit Network Selection TTCN Tree and T abular Combined Notation UNI User-Network Interface VCI Virtual Channel Identifier VPI Virtual Path Identifier

Page 5-2

Abstract Test Suite for UNI 3.1 Signalling for the Network Side af-test-0090.000

ATM Forum Technical Committee

6. References

[1] “ATM User-Network Interface Specification, Version 3.1”, ATM Forum, 1995.

[2] ISO/IEC 9646-3: 1990, Information Technology - Open Systems Interconnection - Conformance Testing Methodology and Framework - Part 3 Tree and Tabular Combined Notation (See also CCITT Recommendation X.292 (1991))

[3] ISO/IEC 9646-2: 1990, Information Technology - Open Systems Interconnection - Conformance Testing Methodology and Framework - Part 2 Abstract Test Suite Specification. (See also CCITT Recommendation X.291(1991))

[4] ISO/IEC 9646-1: 1990, Information Technology - Open Systems Interconnection - Conformance Testing Methodology and Framework - Part 1: General Concepts. (See also CCITT Recommendation X.290 (1991))

Page 6-1

Annex A

ATM UNI 3.1 Signalling Conformance PIXIT Proforma

ATM UNI 3.1 Signalling PIXIT - For Network Side

Abstract Test Suite Manual A-3

ATM UNI 3.1 Signalling PIXIT Proforma For Network Side IUT Name: ________________________________________________________________________________

Version: ______________________________________________________________________________

Machine Configuration: _________________________________________________________________

Operating System Identification: _________________________________________________________

IUT Identification: ______________________________________________________________________

PICS Reference for IUT : _________________________________________________________________

Limitations of the IUT : __________________________________________________________________

ATM UNI 3.1 Signalling PIXIT - For Network Side

A-4 Abstract Test Suite Manual

Instructions for Completing the PIXIT Proforma

The Protocol Implementation eXtra Information for Testing (PIXIT) is a document which is to be completed by the user submitting an implementation for testing. It contains information related to the Implementation Under Test (IUT) and the test environment which is required by the IUT. The PIXIT information is beyond that provided by the Protocol Implementation Conformance Statement (PICS).

This section contains the PIXIT Proforma which meets the requirements of this test suite. The test suite developer and/or test laboratory may provide additional questions to this proforma, as needed.

The user should fill in all sections that are applicable to the implementation, and leave blank those that are not. This is done by either checking a ballot box, or by writing an answer in the provided space. In some cases the type of value to be provided is specified (e.g., a decimal number) along with the proper units (e.g., seconds). When the user is required to check a ballot box and more than one alternative value is listed, the first listed alternative value shall be considered to be the default value for the corresponding PIXIT parameter, unless otherwise indicated in the corresponding Question or Value fields. For a more detailed meaning for each of the possible value choices, the user may refer to ATM Forum "ATM User-Network Interface Specification. Version 3.1".

ATM UNI 3.1 Signalling PIXIT - For Network Side

Abstract Test Suite Manual A-5

Configuration

Item # Question Value Answer

C.1 IUT execute restart procedure at the initialization phase

True, False Default: True

C.2 IUT can be configured with all virtual channels busy. True, False Default: False

True

False

True

False

ATM UNI 3.1 Signalling PIXIT - For Network Side

A-6 Abstract Test Suite Manual

Timers

Item # Question Value Answer

T.1 Value (seconds) for a timer that is sufficiently long for the IUT to respond. It is used when a response is expected from the IUT

Units: seconds Default: 5 s

T.2 Value (seconds) for a timer that is shorter than the shortest IUT implemented timer. It is used when no reponse is expected from the IUT

Units: seconds Default: 3 s

TV.1

Value (seconds) for the IUT T303 timer. It is used for retransmission of SETUP message

Units: seconds Default: 4 s

TV.2

Value (seconds) for the IUT T308 timer. It is used for retransmission of RELEASE message

Units: seconds Default: 30 s

TV.3 Value (seconds) for the IUT T309 timer. It is used during a SAAL disconnection

Units: seconds Default: 10 s

TV.4

Value (seconds) for the IUT T310 timer. It is used when the CALL PROCEEDING message is received

Units: seconds Default: 10 s

TV.5

Value (seconds) for the IUT T322 timer. It is used when the STATUS ENQUIRY message is sent

Units: seconds Default: 4 s

TV.6

Value (seconds) for a timer tolerance. (the delay time in transferring and processing messages)

Units: seconds Default: 1 s

ATM UNI 3.1 Signalling PIXIT - For Network Side

Abstract Test Suite Manual A-7

Options

Item # Question Value Answer

O.1 IUT generates a CALL PROCEEDING after receiving a SETUP from the user

True, False Default: False

O.2 IUT generates a STATUS after a message with a Non-Mandatory IE error

True, False Default: False

O.3 IUT generates a STATUS ENQUIRY after a SAAL Link error

True, False Default: False

O.4 IUT resends SETUP after the expiry of timer T303

True, False Default: False

O.5 IUT requires the Calling Party Number in the SETUP Message

True, False Default: False

O.6 IUT follows Action Indicator when Message Type Octet 2 Flag =1

True, False Default: False

O.7 IUT supports the Broadband High Layer Information Element

True, False Default: True

O.8 IUT supports the repetition of Broadband Low layer Information Element

True, False Default: True

O.9 IUT transports the Broadband Low Layer Information Element to the calling user in CONNECT message

True, False Default: True

O.10 IUT supports the Transit Network Selection Information Element

True, False Default: True

O.11

Choose a valid Transit Network Selection identification code (a carrier identification code) .(Note 1)

IA5 characters Default: 0000

True

False

True

False

True

False

True

False

True

False

True

False

True

False

True

False

True

False

True

False

ATM UNI 3.1 Signalling PIXIT - For Network Side

A-8 Abstract Test Suite Manual

O.12 Choose an unrecognized Transit Network Selection identification code.(Note 1)

IA5 characters Default: 0000

O.13 Choose a non valid Transit Network Selection identification code .(Note 1)

IA5 characters Default: 0000

Note 1: the response is meaningful only if O.10 is True.

Item # Question Value Answer

ATM UNI 3.1 Signalling PIXIT - For Network Side

Abstract Test Suite Manual A-9

Traffic

Item # Field Binary Value Meaning

TR.1 Bearer Class A is supported

True, False Default: True

TR.2 Bearer Class C is supported

True, False Default:True

TR.3 Bearer Class X (CBR) is supported

True, False Default:True

TR.4 Bearer Class X (VBR) is supported

True, False Default:True

TR.5 Peak Cell Rate (CLP = 0+1)

Integer Default:328

TR.6 Peak Cell Rate (CLP=0) is supported True, False Default:False

TR.7 Peak Cell Rate (CLP = 0)(Note 1)

Integer Default:164

TR.8 SCR and MBS (CLP=0) are supported True, False Default:False

TR.9 Sustainable Cell Rate (CLP = 0)(Note 2)

Integer Default:41

TR.10 Maximum Burst Size (CLP = 0)(Note 2)

Integer Default:32

TR.1 SCR and MBS (CLP=0+1) are supported True, False Default:False

TR.12

Sustainable Cell Rate (CLP = 0+1)(Note 3)

Integer Default:82

True

False

True

False

True

False

True

False

True

False

True

False

True

False

ATM UNI 3.1 Signalling PIXIT - For Network Side

A-10 Abstract Test Suite Manual

TR.13 Maximum Burst Size (CLP = 0+1)(Note 3)

Integer Default:32

TR.14 Best Effort is supported

True, False Default:True

TR.15 QoS Class 1 is supported

True, False Default:True

TR.16 QoS Class 3 is supported

True, False Default:True

Note 1: the response is meaningful only if TR.6 is True. Note 2: the response is meaningful only if TR.8 is True. Note 3: the response is meaningful only if TR.11 is True.

Item # Field Binary Value Meaning

True

False

True

False

True

False

ATM UNI 3.1 Signalling PIXIT - For Network Side

Abstract Test Suite Manual A-11

Addresses

Item # Question Value Answer

A.1 Public (E.164) format or Private (NSAP) for- mat Public, Private

Default:Private

A.2 Address of T Port^{(Note 1)} Hexstring

A.3 Address of R1 port^{(Note 1)} Hexstring

A.4 Invalid Address(Note 1) Hexstring

A.5 Address of T Port in Called Party Number sent in outgoing SETUP from R1(Note 2)

IA5 characters

A.6 Address of T Port in Called Party Number received in incoming SETUP at T(Note 2)

IA5 characters

A.7 Address of T Port in Calling Party Number sent in outgoing SETUP from T(Note 2)

IA5 characters

A.8 Address of R1Port in Called Party Number sent in outgoing SETUP from T(Note 2)

IA5 characters

A.9 Address of R1 Port in Calling Party Number sent in outgoing SETUP from R1(Note 2)

IA5 characters

A.10 Address of R1 Port in Calling Party Number received in incoming SETUP at T(Note 2)

IA5 characters

A.1 Invalid Address(Note 2) IA5 characters

Note 1: the response is meaningful only if A.1 is Private.

Note 2: the response is meaningful only if A.1 is Public.

Public (E.164)

Private (NSAP)

Annex B

ATM Forum UNI 3.1 Signalling Conformance Test Matrix

ATM/Forum 95-0868R3

ATM Forum Technical Committee B-3

Table of Contents

Section Page Number

Introduction B-5

General - Outgoing B-7

General - Incoming B-15

General - Clearing B-19

Error - General B-26 Protocol Discriminator Error B-26 Message too short B-28 Message length error B-30 IE. duplicated more than the specification B-32 Message Type Octet 2 Flag=1 B-39

Error - Call Reference B-45 Non-zero bits 5-8 octet 1 B-45 Length not equal to 3 B-47 Value not in use B-49 Flag incorrectly set to 1... B-50 Global call reference B-51

Error - Message Sequence B-53

Error - Mandatory B-58 Mandatory IE. missing B-58 Mandatory IE. invalid content B-60

Error - Non-Mandatory B-71 Unrecognized IE. B-71 IE. content error B-78 Unexpected recognized IE. B-97

Error - AAL Reset B-105

Error - AAL Failure B-107

Timers B-108

Status Enquiry Procedure B-111

Notes B-113

Legend B-115

Introduction

ATM Forum Technical Committee B-5

Introduction

The matrix describes the test purposes and scenarios in terms of an event, state, and response that may lead the IUT to a new state. Each event has a unique number and event qualifier describing the major characteristics of that event (i.e. the information elements that need to be included in a message being sent to the IUT). Similarly, a response is associated with a qualifier that describes the major characteristics of that response (i.e. the information elements that should be included in an expected message from the IUT). The new state field indicates the IUT state following the state transition defined by the indicated event and the associated response. The test can be classified as being Valid, Not valid, or Inopportune, depending on the event type and characteristics.

The “=” sign is often used to express the content details of an information element (i.e. CA/value = 100).

Each row of the matrix may describe one or more tests that are based on the same event (left most column of the matrix). However, each test requires the event to be invoked at a different state, referred to as “the current state” (first row, following the header, of the matrix) and leads the IUT to the next state, referred to as “the new state”. The following line diagram shows the intended interpretation of the tests defined by the matrix.

As an example, consider the test specification given below. The current state is N6 and the event consists of a CONNECT (CONN) message being sent to the Implementation Under Test (IUT). The response from the IUT is CONNECT ACKNOWLEDGE (CONN ACK). The new state becomes N10. This test case is classified as a Valid test.

Event Call Present SN: N6 E: CONN EQ:

Event:

R: CONN ACK RQ:

NS: N10 Class: V(5.5.2.7)

Event (E)

Response (R)

IUT Tester

New State (NS)

Current State (CS)

Introduction

B-6 ATM Forum Technical Committee

The successful execution of the above test case is captured in the following line diagram.

IUT Tester

R: CONN ACK

E:CONN CS:N6

NS:N10

B-7 ATM Forum Technical Committee

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12} E: SETUP EQ: Note 1,2,4,21.

Event: 1

R: NO RESPONSE

NS: N1 Class: V(5.5.1.5) E: SETUP EQ: Note 1,3,4,21.

Event: 1

R: CALL PROC RQ: with a valid CI. NS: N3 Class: V(5.5.1.5) E: SETUP EQ: with AALP. Note 2,5,21.

Event: 2

R: NO RESPONSE

NS: N1 Class: V(5.5.1.5) E: SETUP EQ: with AALP. Note 3,5,21.

Event: 2

R: CALL PROC RQ: with a valid CI. NS: N3 Class: V(5.5.1.5) E: SETUP EQ: with BHL. Note 2,5,7,21.

Event: 3

R: NO RESPONSE

NS: N1 Class: V(5.5.1.5)

General-Outgoing

ATM Forum Technical Committee B-8

E: SETUP EQ: with BHL. Note 3,5,7,21.

Event: 3

R: CALL PROC RQ: with a valid CI. NS: N3 Class: V(5.5.1.5) E: SETUP EQ: with BLL. Note 2,5,21.

Event: 4

R: NO RESPONSE.

NS: N1 Class: V(5.5.1.5) E: SETUP EQ: with BLL. Note 3,5,21 .

Event: 4

R: CALL PROC RQ: with a valid CI. NS: N3 Class: V(5.5.1.5) E: SETUP EQ: with BRI and BLL. Note 2,5,21.

Event: 5

R: NO RESPONSE

NS: N1 Class: V(5.5.1.5) E: SETUP EQ: with BRI and BLL. Note 3,5,21.

Event: 5

R: CALL PROC RQ: with a valid CI. NS: N3 Class: V(5.5.1.5)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

General-Outgoing

B-9 ATM Forum Technical Committee

E: SETUP EQ: with BRI and 2 BLL. Note 2,5 ,9,21.

Event: 6

R: NO RESPONSE

NS: N1 Class: V(5.5.1.5) E: SETUP EQ: with BRI and 2 BLL. Note 3,5,9,21.

Event: 6

R: CALL PROC RQ: with a valid CI. NS: N3 Class: V(5.5.1.5) E: SETUP EQ: with CDS. Note 2,5,21,30.

Event: 7

R: NO RESPONSE

NS: N1 Class: V(5.5.1.5) E: SETUP EQ: with CDS. Note 3,5,21,30.

Event: 7

R: CALL PROC RQ: with a valid CI. NS: N3 Class: V(5.5.1.5) E: SETUP EQ: with CGS. Note 2,5,21,30.

Event: 8

R: NO RESPONSE

NS: N1 Class: V(5.5.1.5)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

General-Outgoing

ATM Forum Technical Committee B-10

E: SETUP EQ: with CGS. Note 3,5,21,30.

Event: 8

R: CALL PROC RQ: with a valid CI. NS: N3 Class: V(5.5.1.5) E: SETUP EQ: without CGN. Note 2,5.

Event: 9

R: NO RESPONSE

NS: N1 Class: V(5.5.1.5) E: SETUP EQ: without CGN. Note 3,5.

Event: 9

R: CALL PROC RQ: with a valid CI. NS: N3 Class: V(5.5.1.5) E: SETUP EQ: with CGN. Note 2,5.

Event: 10

R: NO RESPONSE

NS: N1 Class: V(5.5.1.5) E: SETUP EQ: with CGN. Note 3,5.

Event: 10

R: CALL PROC RQ: with a valid CI. NS: N3 Class: V(5.5.1.5)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

General-Outgoing

B-11 ATM Forum Technical Committee

E: SETUP EQ: with BSC. Note 2,5,21.

Event: 11

R: NO RESPONSE

NS: N1

Class: V(5.5.1.5) E: SETUP EQ: with BSC. Note 3,5,21

Event: 11

R: CALL PROC RQ: with a valid CI. NS: N3 Class: V(5.5.1.5) E: SETUP EQ: with TNS. Note 2,5,11,21.

Event: 12

R: NO RESPONSE

NS: N1

Class: V(5.5.1.5) E: SETUP EQ: with TNS. Note 3,5,11,21.

Event: 12

R: CALL PROC RQ: with a valid CI. NS: N3 Class: V(5.5.1.5) E: remote CONN EQ: without any optional IE. Note 1,3.

Event: 13

R: CONN RQ: without CI. NS: N10 Class: V(5.5.1.7)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

General-Outgoing

ATM Forum Technical Committee B-12

E: remote CONN

EQ: without any optional IE. Note 1,2.

Event: 13

R: CONN RQ: with CI.

NS: N10 Class: V(5.5.1.7) E: remote CONN

EQ: with AALP. Note 3,12.

Event: 14

R: CONN

RQ: with AALP and without CI. NS: N10 Class: V(5.5.1.7) E: remote CONN

EQ: with AALP. Note 2,12.

Event: 14

R: CONN

RQ: with AALP and CI. NS: N10 Class: V(5.5.1.7) E: remote CONN

EQ: without AALP. Note 3,12.

Event: 15

R: CONN

RQ: without AALP and CI. NS: N10 Class: V(5.5.1.7) E: remote CONN

EQ: without AALP. Note 2,12.

Event: 15

R: CONN

RQ: with CI and without AALP. NS: N10 Class: V(5.5.1.7)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

General-Outgoing

B-13 ATM Forum Technical Committee

E: remote CONN EQ: with BLL. Note 3,13,15.

Event: 16

R: CONN RQ: with BLL and without CI. NS: N10 Class: V(5.5.1.7) E: remote CONN EQ: with BLL. Note 2,13,15.

Event: 16

R: CONN RQ: with BLL and CI. NS: N10 Class: V(5.5.1.7) E: remote CONN EQ: with BLL. Note 3,13,14.

Event: 17

R: CONN RQ: without BLL and CI. NS: N10 Class: V(5.5.1.7) E: remote CONN EQ: with BLL. Note 2,13,14.

Event: 17

R: CONN RQ: without BLL and with CI. NS: N10 Class: V(5.5.1.7) E: remote CONN EQ: without BLL. Note 3,13.

Event: 18

R: CONN RQ: without BLL and CI. NS: N10 Class: V(5.5.1.7)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

General-Outgoing

ATM Forum Technical Committee B-14

E: remote CONN

EQ: without BLL. Note 2,13.

Event: 18

R: CONN RQ: without BLL and with CI.

NS: N10 Class: V(5.5.1.7) E: CONN ACK

EQ: Note 16.

Event: 19

R: NO RESPONSE

NS: N10 Class: V(5.5.1.7)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

General-Outgoing

B-15 ATM Forum Technical Committee

E: remote SETUP

EQ: Note 1,5,21.

Event: 51

R: SETUP start T303N RQ: with a valid CI. Note 17,18.

NS: N6 Class: V(5.5.2.1)

E: remote SETUP

EQ: with AALP. Note 5,21.

Event: 52

R: SETUP start T303N RQ: with a valid CI and AALP. Note 17,18.

NS: N6 Class: V(5.5.2.1)

E: remote SETUP

EQ: with BHL. Note 5,7,21.

Event: 53

R: SETUP start T303N RQ: with a valid CI and BHL. Note 17,18.

NS: N6 Class: V(5.5.2.1)

E: remote SETUP

EQ: with BLL. Note 5,21.

Event: 54

R: SETUP start T303N RQ: with a valid CI and BLL. Note 17,18.

NS: N6 Class: V(5.5.2.1)

E: remote SETUP

EQ: with BRI and BLL. Note 5,21.

Event: 55

R: SETUP start T303N RQ: with a valid CI and BLL (may be BRI). Note 17,18. NS: N6 Class: V(5.5.2.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix

Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

General-Incoming

ATM Forum Technical Committee B-16

E: remote SETUP

EQ: with BRI and 2 BLL. Note 5,9,21.

Event: 56

R: SETUP start T303N RQ: with a valid CI, BRI and 2 BLL. Note 17,18. NS: N6 Class: V(5.5.2.1) E: remote SETUP

EQ: with CDS. Note 5,21,30.

Event: 57

R: SETUP start T303N RQ: with a valid CI and CDS. Note 17,18.

NS: N6 Class: V(5.5.2.1)

E: remote SETUP

EQ: with CGS.Note 5,21,30.

Event: 58

R: SETUP start T303N RQ: with a valid CI, and CGS.Note 17,18.

NS: N6 Class: V(5.5.2.1)

E: remote SETUP

EQ: without CGN . Note 5.

Event: 59

R: SETUP start T303N RQ: with a valid CI. Note 17,18.

NS: N6 Class: V(5.5.2.1)

E: remote SETUP

EQ: with CGN. Note 5. Event: 60

R: SETUP start T303N RQ: with a valid CI. Note 17,18.

NS: N6 Class: V(5.5.2.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix

Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

General-Incoming

B-17 ATM Forum Technical Committee

E: remote SETUP

EQ: with BSC. Note 5,21.

Event: 61

R: SETUP start T303N RQ: with a valid CI. Note 17,18. NS: N6 Class: V(5.5.2.1) E: remote SETUP

EQ: with TNS. Note 5,11,21.

Event: 62

R: SETUP start T303N RQ: with a valid CI and without TNS. Note 17,18. NS: N6 Class: V(5.5.2.1) E: CALL PROC

EQ: with CI same as the last SETUP.

Event: 63

R: NO RESPONSE stop T303N, start T310N

NS: N9

Class: V(5.5.2.5.2) E: CALL PROC

EQ: without CI.

Event: 64

R: NO RESPONSE stop T303N, start T310N

NS: N9

Class: V(5.5.2.5.2) E: CONN

EQ: with CI same as the last SETUP. Note 1.

Event: 65

R: CONN ACK stop T303N

NS: N10 Class: V(5.5.2.7)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

General-Incoming

ATM Forum Technical Committee B-18

E: CONN

EQ: without CI. Note 1. Event: 66

R: CONN ACK stop T303N

NS: N10 Class: V(5.5.2.7)

R: CONN ACK stop T310N

NS: N10 Class: V(5.5.2.7) E: CONN

EQ: without CI and with AALP. Note 12.

Event: 67

R: CONN ACK stop T303N

NS: N10 Class: V(5.5.2.7)

R: CONN ACK stop T310N

NS: N10 Class: V(5.5.2.7) E: CONN

EQ: without CI and without AALP. Note 12. Event: 68

R: CONN ACK stop T303N

NS: N10 Class: V(5.5.2.7)

R: CONN ACK stop T310N

NS: N10 Class: V(5.5.2.7) E: CONN

EQ: without CI and with BLL. Note 13,15.

Event: 69

R: CONN ACK stop T303N

NS: N10 Class: V(5.5.2.7)

R: CONN ACK stop T310N

NS: N10 Class: V(5.5.2.7) E: CONN

EQ: without CI and without BLL. Note 13.

Event: 70

R: CONN ACK stop T303N

NS: N10 Class: V(5.5.2.7)

R: CONN ACK stop T310N

NS: N10 Class: V(5.5.2.7)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

General-Incoming

B-19 ATM Forum Technical Committee

E: SETUP EQ: (local clearing). Network have no vci in any vpci available. Note 1,5,19,21. Event: 101

R: RELEASE COMP

RQ: CA/value = 45. NS: N0

Class: V(5.5.1.2.1) E: SETUP

EQ: (local clearing). QOS class not provided by network. Note 1,21. Event: 102

R: RELEASE COMP

RQ: CA/value = 49. NS: N0

Class: V(5.5.1.3) E: SETUP

EQ: (local clearing). ATD not provided by network. Note 1,21. Event: 103

R: RELEASE COMP

RQ: CA/value = 37,51. NS: N0

Class: V(5.5.1.3) E: SETUP EQ: (local clearing). Non supported set of traffic parameters. Note 1,21. Event: 104

R: RELEASE COMP

RQ: CA/value = 73. NS: N0

Class: V(5.5.1.3) E: SETUP EQ: (local clearing). Requested service not available (BBC Class). Note 1,2,21.

Event: 105

R: RELEASE COMP RQ:CA/value = 57,58, 63,65 NS: N0

Class: V(5.5.1.5)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

General-Clearing

ATM Forum Technical Committee B-20

E: SETUP EQ: (local clearing). Requested service not available (BBC Class). Note 1,3,21.

Event: 105

R: CALL PROC + RELEASE start T308N RQ:CA/value = 57,58, 63,65. NS: N12 Class: V(5.5.1.5) E: remote RELEASE COMP EQ: (remote clearing). CA/value = 35. Note 2.

Event: 106

R: RELEASE COMP

RQ: CA/value = 41,35.

NS: N0 Class: V(5.5.2.3)

E: remote RELEASE COMP EQ: (remote clearing). CA/value= 35. Note 3.

Event: 106

R: RELEASE start T308N

RQ: CA/value = 41,35.

NS: N12 Class: V(5.5.2.3) E: remote CALL

PROC EQ: (remote clearing). vpci and vci are not the same as SETUP. Note 2. Event: 107

R: RELEASE COMP

RQ: CA/value = 41,36.

NS: N0

Class: V(5.5.2.3) E: remote CALL

PROC EQ: (remote clearing). vpci and vci are not the same as SETUP. Note 3. Event: 107

R: RELEASE start T308N

RQ: CA/value = 41,36.

NS: N12 Class: V(5.5.2.3)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

General-Clearing

B-21 ATM Forum Technical Committee

E: remote RELEASE COMP EQ: (remote clearing). CA/value = 49. with diagnostic (8CH). Note 2 . Event: 108

R: RELEASE COMP

RQ: CA/value = 49.

NS: N0

Class: V(5.5.2.4) E: remote RELEASE COMP EQ: (remote clearing). CA/value = 49. with diagnostic (8CH). Note 3.

Event: 108

R: RELEASE start T308N

RQ: CA/value = 49.

NS: N12 Class: V(5.5.2.4) E: remote RELEASE COMP EQ: (remote clearing). CA/value = 47. Note 2.

Event: 109

R: RELEASE COMP

RQ: CA/value = 47.

NS: N0

Class: V(5.5.2.4) E: remote RELEASE COMP EQ: (remote clearing). CA/value = 47. Note 3.

Event: 109

R: RELEASE start T308N

RQ: CA/value = 47.

NS: N12 Class: V(5.5.2.4) E: remote RELEASE COMP EQ: (remote clearing). CA/value = 88. with diagnostic (70H). Note 2.

Event: 110

R: RELEASE COMP

RQ: CA/value = 88.

NS: N0

Class: V(5.5.2.5.1.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

General-Clearing

ATM Forum Technical Committee B-22

E: remote RELEASE COMP EQ: (remote clearing). CA/value = 88. with diagnostic (70H). Note 3.

Event: 110

R: RELEASE start T308N

RQ: CA/value = 88.

NS: N12 Class: V(5.5.2.5.1.1)

E: remote RELEASE COMP EQ: (remote clearing). CA/value = 17. Note 2.

Event: 111

R: RELEASE COMP

RQ: CA/value = 17.

NS: N0

Class: V(5.5.2.5.1.1) E: remote RELEASE COMP EQ: (remote clearing). CA/value = 17. Note 3.

Event: 111

R: RELEASE start T308N

RQ: CA/value = 17.

NS: N12 Class: V(5.5.2.5.1.1) E: remote RELEASE COMP EQ: (remote clearing). CA/value = 21.with diagnostic (80FFH). Note 2. Event: 112

R: RELEASE COMP

RQ: CA/value = 21.

NS: N0

Class: V(5.5.2.5.1.1) E: remote RELEASE COMP EQ: (remote clearing). CA/value = 21. with diagnostic (80FFH). Note 3. Event: 112

R: RELEASE start T308N

RQ: CA/value = 21.

NS: N12 Class: V(5.5.2.5.1.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

General-Clearing

B-23 ATM Forum Technical Committee

E: remote RELEASE COMP EQ: (remote clearing). CA/value = 23, CA/ coding =11B. Note 2,20. Event: 113

R: RELEASE COMP

RQ: CA/value = 23, CA/coding =11B. NS: N0

Class: V(5.5.2.5.1.1) E: remote RELEASE COMP EQ: (remote clearing). CA/value = 23, CA/ coding =11B. Note 3,20. Event: 113

R: RELEASE start T308N RQ: CA/value = 23, CA/coding =11B. NS: N12 Class: V(5.5.2.5.1.1)

E: CALL PROC EQ: ( local clearing) with CI (vpci,cvi are not the same as the last SETUP).

Event: 114

R: RELEASE stop T303N, start T308N RQ: CA/value = 36. NS: N12

Class: V(5.5.2.3) E: RELEASE

EQ: (local clearing). CA/value = 16. Note 2.

Event: 115

R: RELEASE COMP

NS: N0

Class: V(5.5.4.3) E: RELEASE

EQ: (local clearing). CA/value = 16. Note 3.

Event: 115

R: RELEASE COMP

NS: N0

Class: V(5.5.4.3)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

General-Clearing

ATM Forum Technical Committee B-24

E: RELEASE

EQ: (local clearing). CA/value = 16.

Event: 116

R: RELEASE COMP stop T310N

NS: N0 Class: V(5.5.4.3)

R: RELEASE COMP

NS: N0 Class: V(5.5.4.3) E: RELEASE

EQ: CA/value = 16. (collision).

Event: 117

R: NO RESPONSE stop T308N

NS: N0 Class: V(5.5.4.5) E: RELEASE COMP

EQ: CA/value = 41.

Event: 118

R: NO RESPONSE stop T303N

NS: N0 Class: V(5.5.4.2) E: RELEASE COMP

Event: 119

R: NO RESPONSE stop T308N

NS: N0 Class: V(5.5.4.4) E: RESTART

EQ: RI/class = all channels.

Event: 120

R: RESTART ACK

NS: N0 Class: V(5.5.5.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

General-Clearing

B-25 ATM Forum Technical Committee

E: RESTART

EQ: RI/class = all channels.

Event: 121

R: RESTART ACK

NS: N0

Class: V(5.5.5.2) E: RESTART

EQ: RI/class = indicated channel, CI/vpci,vci not in use. Event: 122

R: RESTART ACK

NS: N0 Class: V(5.5.5.2) E: RESTART

EQ: RI/class = indicated channel, CI/vpci,vci in use. Event: 123

R: RESTART ACK

NS: N0 Class: V(5.5.5.2)

R: RESTART ACK

NS: N0 Class: V(5.5.5.2)

R: RESTART ACK

NS: N0 Class: V(5.5.5.2)

R: RESTART ACK

NS: N0 Class: V(5.5.5.2) E: RESTART

EQ: RI/class =indicated channel, CI/vpci,vci in use. Note 3. Event: 124

R: RESTART ACK

NS: N0 Class: V(5.5.5.2) E: remote RESTART

EQ: RI/class =all channels.

Event: 125

R: RELEASE start T308N RQ: CA/value = 41.

NS: N12 Class: V(5.5.5.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

General-Clearing

ATM Forum Technical Committee B-26

E: SETUP EQ: protocol discriminator error. Note 1,21.

Event: 151

R: NO RESPONSE

NS: N0 Class: N(5.5.6.1) E: CALL PROC EQ: protocol discriminator error. without CI.

Event: 152

R: NO RESPONSE

NS: N6 Class: N(5.5.6.1) E: CONN EQ: protocol discriminator error. without CI. Event: 153

R: NO RESPONSE

NS: N9 Class: N(5.5.6.1) E: CONN ACK EQ: protocol discriminator error. Note 16.

Event: 154

R: NO RESPONSE

NS: N10 Class: N(5.5.6.1) E: RELEASE EQ: protocol discriminator error.CA/value =16. Event: 155

R: NO RESPONSE

NS: N10 Class: N(5.5.6.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-General Protocol Discriminator Error

B-27 ATM Forum Technical Committee

E: RELEASE COMP

EQ: protocol discriminator error.

Event: 156

R: NO RESPONSE

NS: N12 Class: N(5.5.6.1) E: RESTART

EQ: protocol discriminator error.RI/Class = all channels Event: 157

R: NO RESPONSE

NS: N10 Class: N(5.5.6.1) E: RESTART ACK

EQ: protocol discriminator error.RI/class= all channels Event: 158

R: NO RESPONSE

NS: N10 Class: N(5.5.6.1) E: STATUS

EQ: protocol discriminator error.CS/state =U10, CA/value =30. Event: 159

R: NO RESPONSE

NS: N10 Class: N(5.5.6.1) E: STATUS ENQ

EQ: protocol discriminator error.

Event: 160

R: NO RESPONSE

NS: N10 Class: N(5.5.6.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-General Protocol Discriminator Error

ATM Forum Technical Committee B-28

E: SETUP EQ: message too short (7 octets).

Event: 181

R: NO RESPONSE

NS: N0 Class: N(5.5.6.2) E: CALL PROC EQ: message too short (7 octets).

Event: 182

R: NO RESPONSE

NS: N6 Class: N(5.5.6.2) E: CONN EQ: message too short (7 octets).

Event: 183

R: NO RESPONSE

NS: N9 Class: N(5.5.6.2) E: CONN ACK EQ: message too short (7 octets). Note 16.

Event: 184

R: NO RESPONSE

NS: N10 Class: N(5.5.6.2) E: RELEASE EQ: message too short (7 octets).

Event: 185

R: NO RESPONSE

NS: N10 Class: N(5.5.6.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-General Message too short

B-29 ATM Forum Technical Committee

E: RELEASE COMP EQ: message too short (7 octets).

Event: 186

R: NO RESPONSE

NS: N12 Class: N(5.5.6.2) E: RESTART EQ: message too short (7 octets).

Event: 187

R: NO RESPONSE

NS: N10 Class: N(5.5.6.2) E: RESTART ACK EQ: message too short (7 octets).

Event: 188

R: NO RESPONSE

NS: N10 Class: N(5.5.6.2) E: STATUS EQ: message too short (7 octets).

Event: 189

R: NO RESPONSE

NS: N10 Class: N(5.5.6.2) E: STATUS ENQ EQ: message too short (7 octets).

Event: 190

R: NO RESPONSE

NS: N10 Class: N(5.5.6.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-General Message too short

ATM Forum Technical Committee B-30

E: SETUP

EQ: message length error. Note 1,2,5,21.

Event: 211

R: NO RESPONSE

NS: N1 Class: I(5.5.6.5) E: SETUP

EQ: message length error. Note 1,3,5,21.

Event: 211

R: CALL PROC

RQ: with a valid CI.

NS: N3 Class: I(5.5.6.5) E: CALL PROC

EQ: message length error. without CI.

Event: 212

R: NO RESPONSE stop T303N, start T310N

NS: N9 Class: I(5.5.6.5) E: CONN

EQ: message length error. without CI. Event: 213

R: CONN ACK stop T310N

NS: N10 Class: I(5.5.6.5) E: CONN ACK

EQ: message length error. Note 16.

Event: 214

R: NO RESPONSE

NS: N10 Class: I(5.5.6.5)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-General Message length error

B-31 ATM Forum Technical Committee

E: RELEASE

EQ: message length error. CA/value = 16.

Event: 215

R: RELEASE COMP

NS: N0 Class: I(5.5.6.5) E: RELEASE COMP

EQ: message length error.

Event: 216

R: NO RESPONSE stop T308N

NS: N0 Class: I(5.5.6.5) E: RESTART

EQ: message length error. RI/calss = all channels. Event: 217

R: RESTART ACK

NS: N0 Class: I(5.5.6.5) E: STATUS EQ: message length error. CS/state = U10, CA/value =30.

Event: 218

R: NO RESPONSE

NS: N10 Class: I(5.5.6.5) E: STATUS ENQ

EQ: message length error.

Event: 219

R: STATUS RQ: CA/value = 30, CS/state = N10.

NS: N10 Class: I(5.5.6.5)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-General Message length error

ATM Forum Technical Committee B-32

E: SETUP

EQ: duplicated IE. Note 2,5,21,22.

Event: 241

R: NO RESPONSE

NS: N1 Class: I(5.5.6.6.2) E: SETUP

EQ: duplicated IE. Note 3,5,21,22.

Event: 241

R: CALL PROC

RQ: with a valid CI.

NS: N3 Class: I(5.5.6.6.2) E: SETUP

EQ: duplicated IE. Note 2,5,23.

Event: 242

R: NO RESPONSE

NS: N1 Class: I(5.5.6.6.2) E: SETUP

EQ: duplicated IE. Note 3,5,23.

Event: 242

R: CALL PROC

RQ: with a valid CI.

NS: N3 Class: I(5.5.6.6.2) E: SETUP

EQ: duplicated CGS, CDS IE.Note 2,5,21, 30. Event: 243

R: NO RESPONSE

NS: N1 Class: I(5.5.6.6.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-General IE. duplicated more than the specification

B-33 ATM Forum Technical Committee

E: SETUP

EQ: duplicated CDS, CGS IE. Note 3,5,21,30. Event: 243

R: CALL PROC

RQ: with a valid CI.

NS: N3 Class: I(5.5.6.6.2) E: SETUP

EQ: duplicated IE. Note 2,5,7,21,24.

Event: 244

R: NO RESPONSE

NS: N1 Class: I(5.5.6.6.2) E: SETUP

EQ: duplicated IE. Note 3,5,7,21,24.

Event: 244

R: CALL PROC

RQ: with a valid CI.

NS: N3 Class: I(5.5.6.6.2) E: SETUP

EQ: duplicated IE. Note 2,5,9,21,25.

Event: 245

R: NO RESPONSE

NS: N1 Class: I(5.5.6.6.2) E: SETUP

EQ: duplicated IE. Note 3,5,9,21,25.

Event: 245

R: CALL PROC

RQ: with a valid CI.

NS: N3 Class: I(5.5.6.6.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-General IE. duplicated more than the specification

ATM Forum Technical Committee B-34

E: SETUP

EQ: duplicated IE. Note 2,5,21,26.

Event: 246

R: NO RESPONSE

NS: N1 Class: I(5.5.6.6.2) E: SETUP

EQ: duplicated IE. Note 3,5,21,26.

Event: 246

R: CALL PROC

RQ: with a valid CI.

NS: N3 Class: I(5.5.6.6.2) E: SETUP

EQ: duplicated IE. Note 2,5,11,21,27.

Event: 247

R: NO RESPONSE

NS: N1 Class: I(5.5.6.6.2)

E: SETUP

EQ: duplicated IE. Note 3,5,11,21,27.

Event: 247

R: CALL PROC

RQ: with a valid CI.

NS: N3 Class: I(5.5.6.6.2) E: remote SETUP

EQ: duplicated IE. Note 21,22. Event: 248

R: SETUP strat T303N RQ: with a valid CI. Note 17,18. NS: N6 Class: I(5.5.6.6.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-General IE. duplicated more than the specification

B-35 ATM Forum Technical Committee

E: remote SETUP

EQ: duplicated IE. Note 23.

Event: 249

R: SETUP start T303N RQ: with a valid CI, AALP. Note 17,18.

NS: N6 Class: I(5.5.6.6.2) E: remote SETUP

EQ: duplicated CGS CDS IE. Note 21,30.

Event: 250

R: SETUP start T303N RQ: with a valid CI, CDS,CGS. Note 17,18. NS: N6

Class: I(5.5.6.6.2) E: remote SETUP

EQ: duplicated IE. Note 7,21,24.

Event: 251

R: SETUP start T303N RQ: with a valid CI and BHL. Note 17,18.

NS: N6 Class: I(5.5.6.6.2) E: remote SETUP

EQ: duplicated IE. Note 9,21,25.

Event: 252

R: SETUP start T303N RQ: with a valid CI, BRI and 3 BLL. Note 17,18. NS: N6 Class: I(5.5.6.6.2) E: remote SETUP

EQ: duplicated IE. Note 21,26.

Event: 253

R: SETUP start T303N RQ: with a valid CI. Note 17,18. NS: N6 Class: I(5.5.6.6.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix

Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-General IE. duplicated more than the specification

ATM Forum Technical Committee B-36

E: remote SETUP

EQ: duplicated IE. Note 11,21,27.

Event: 254

R: SETUP start T303N RQ: with a valid CI and without TNS. Note 17,18 NS: N6 Class: I(5.5.6.6.2) E: CALL PROC EQ: duplicated IE. (CI).

Event: 255

R: NO RESPONSE stop T303N, start T310N NS: N9

Class: I(5.5.6.6.2)

E: CONN

EQ: duplicated IE. (AALP). Note 12.

Event: 256

R: CONN ACK stop T303N

NS: N10

Class: I(5.5.6.6.2)

E: CONN

EQ: duplicated IE. (BLL 4 times). Note 13,15. Event: 257

R: CONN ACK stop T303N

NS: N10 Class: I(5.5.6.6.2.)

E: remote CONN

EQ: duplicated IE. (AALP). Note 3,12.

Event: 258

R: CONN RQ: with AALP and without CI.

NS: N10 Class: I(5.5.6.6.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-General IE. duplicated more than the specification

B-37 ATM Forum Technical Committee

E: remote CONN

EQ: duplicated IE. (AALP). Note 2,12.

Event: 258

R: CONN RQ: with AALP and CI. NS: N10 Class: I(5.5.6.6.2) E: remote CONN

EQ: duplicated IE. (BLL 4 times). Note 3,13,15. Event: 259

R: CONN RQ: with BLL and without CI.

NS: N10 Class: I(5.5.6.6.2.)

E: remote CONN

EQ: duplicated IE. (BLL 4 times). Note 2,13,15. Event: 259

R: CONN RQ: with BLL and CI.

NS: N10 Class: I(5.5.6.6.2.)

E: RELEASE COMP

EQ: duplicated IE. (CA:3 times ).CA/value = 41. Event: 260

R: NO RESPONSE stop T303N

NS: N0 Class: I(5.5.6.6.2) E: RESTART

EQ: duplicated IE. (RI). RI/Class= all channels. Event: 261

R: RESTART ACK

NS: U0 Class: I(5.5.6.6.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-General IE. duplicated more than the specification

ATM Forum Technical Committee B-38

E: STATUS

EQ:duplicated IE. (CS 2 times). CS/state = U10, CA/value = 30. Event: 262

R: NO RESPONSE

NS: N10 Class: I(5.5.6.6.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-General IE. duplicated more than the specification

B-39 ATM Forum Technical Committee

E: SETUP

EQ: MT/flag = 1 , indicator = 01B, ATD missing. Note 1,21,28. Event: 281

R: NO RESPONSE

NS: N0 Class: I(5.4.4.1)

E: SETUP

EQ: MT/flag = 1 , indicator = 10B, ATD missing. Note 1,21,28. Event: 282

R: STATUS

RQ: CS/state = N0.

NS: N0 Class: I(5.4.4.1) E: SETUP

EQ: MT/flag = 1 , indicator = 01B. Note 1,3,5,21,29. Event: 283

R: CALL PROC

RQ: with a valid CI.

NS: N3 Class: I(5.4.4.1) E: SETUP

EQ: MT/flag = 1 , indicator = 01B. Note 1,2,5,21,29. Event: 283

R: NO RESPONSE

NS: N1 Class: I(5.4.4.1) E: CALL PROC EQ: MT/flag = 1 , indicator = 01B, with unrecognized IE . without CI. Note 28. Event: 284

R: NO RESPONSE

NS: N6 Class: I(5.4.4.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-General Message Type Octet 2 Flag=1

ATM Forum Technical Committee B-40

E: CALL PROC EQ: MT/flag = 1 , indicator = 10B, with unrecognized IE. without CI. Note 28. Event: 285

R: STATUS RQ: CS/state = N6.

NS: N6

Class: I(5.4.4.1) E: CALL PROC EQ: MT/flag = 1 , indicator = 01B, without CI. Note 29. Event: 286

R: NO RESPONSE stop T303N, start T310N

NS: N9

Class: I(5.4.4.1) E: CONN EQ: MT/flag = 1 , indicator = 01B, with unrecognized IE, without CI. Note 1,28. Event: 287

R: NO RESPONSE

NS: N9

Class: I(5.4.4.1) E: CONN EQ: MT/flag = 1 , indicator = 10B, with unrecognized IE, without CI. Note 1,28. Event: 288

R: STATUS RQ: CS/state = N9.

NS: N9

Class: I(5.4.4.1) E: CONN

EQ: MT/flag = 1 , indicator = 01B. without CI. Note 1,29. Event: 289

R: CONN ACK stop T310N

NS: N10 Class: I(5.4.4.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-General Message Type Octet 2 Flag=1

B-41 ATM Forum Technical Committee

E: CONN ACK

EQ: MT/flag = 1 , indicator = 01B. Note 16.

Event: 290

R: NO RESPONSE NS: N10

Class: I(5.4.4.1)

E: CONN ACK

EQ: MT/flag = 1 , indicator = 10B, with unrecognized IE . Note 16,28. Event: 291

R: STATUS RQ: CS/state = N10.

NS: N10

Class: I(5.4.4.1) E: RELEASE EQ: MT/flag = 1 , indicator = 01B. CA/value = 16, with unrecognized IE. Note 28. Event: 292

R: NO RESPONSE

NS: N10

Class: I(5.4.4.1) E: RELEASE EQ: MT/flag = 1 , indicator = 10B. CA/value =16, with unrecognized IE. Note 28. Event: 293

R: STATUS RQ: CS/state = N10

NS: N10

Class: I(5.4.4.1) E: RELEASE

EQ: MT/flag = 1 , indicator = 01B. CA/value = 16. Note 29. Event: 294

R: RELEASE COMP

NS: N0

Class: I(5.4.4.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-General Message Type Octet 2 Flag=1

ATM Forum Technical Committee B-42

E: RELEASE COMP EQ: MT/flag = 1 , indicator = 01B, with unrecognized IE. Note 28. Event: 295

R: NO RESPONSE

NS: N12

Class: I(5.4.4.1) E: RELEASE COMP EQ: MT/flag = 1 , indicator = 10B, with unrecognized IE. Note 28. Event: 296

R: STATUS RQ: CS/state = N12.

NS: N12

Class: I(5.4.4.1) E: RELEASE COMP

EQ: MT/flag = 1 , indicator = 01B. Note 29. Event: 297

R: NO RESPONSE stop T308N

NS: N0 Class: I(5.4.4.1) E: RESTART EQ: MT/flag = 1 , indicator = 01B. RI/class = all channels, with unrecognized IE. Note 28. Event: 298

R: NO RESPONSE

NS: N10

Class: I(5.4.4.1) E: RESTART EQ: MT/flag = 1 , indicator = 10.B. RI/class = all channels, with unrecognized IE . Note 28. Event: 299

R: STATUS RQ: CR/global value. CS/state = Rest 0

NS: N10 Class: I(5.4.4.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-General Message Type Octet 2 Flag=1

B-43 ATM Forum Technical Committee

E: RESTART

EQ: MT/flag = 1 , indicator = 01B. RI/class = all channels. Note 29. Event: 300

R: RESTART ACK

NS: N0

Class: I(5.4.4.1) E: STATUS EQ: MT/flag = 1 , indicator = 01B. CS/state = U10 , CA/value = 30.

Event: 301

R: NO RESPONSE

NS: N10

Class: I(5.4.4.1) E: STATUS EQ: MT/flag = 1 , indicator = 10B.CS/state= U10. CA/value = 30, with unrecognized IE. Note 28. Event: 302

R: STATUS RQ: CS/state = N10.

NS: N10

Class: I(5.4.4.1) E: STATUS ENQ EQ: MT/flag = 1 , indicator = 01B, with unrecognized IE. Note 28.

Event: 303

R: NO RESPONSE

NS: N10

Class: I(5.4.4.1) E: STATUS ENQ EQ: MT/flag = 1 , indicator = 10B, with unrecognized IE. Note 28.

Event: 304

R: STATUS RQ: CS/state = N10.

NS: N10

Class: I(5.4.4.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-General Message Type Octet 2 Flag=1

ATM Forum Technical Committee B-44

E: STATUS ENQ

EQ: MT/flag = 1 , indicator = 01B. Note 29.

Event: 305

R: STATUS RQ: CA/value = 30, CS/state = N10.

NS: N10 Class: I(5.4.4.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-General Message Type Octet 2 Flag=1

B-45 ATM Forum Technical Committee

E: SETUP EQ: CR/non-zero bits 5-8. Note 1,21.

Event: 351

R: NO RESPONSE

NS: N0 Class: N(5.5.6.3.1) E: CALL PROC EQ: CR/non-zero bits 5-8. without CI .

Event: 352

R: NO RESPONSE

NS: N6 Class: N(5.5.6.3.1) E: CONN EQ: CR/non-zero bits 5-8. without CI. Event: 353

R: NO RESPONSE

NS: N9 Class: N(5.5.6.3.1) E: CONN ACK EQ: CR/non-zero bits 5-8. Note 16.

Event: 354

R: NO RESPONSE

NS: N10 Class: N(5.5.6.3.1) E: RELEASE EQ: CR/non-zero bits 5-8. CA/value = 16.

Event: 355

R: NO RESPONSE

NS: N10 Class: N(5.5.6.3.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Call Reference non-zero bits 5-8 octet 1

ATM Forum Technical Committee B-46

E: RELEASE COMP EQ: CR/non-zero bits 5-8.

Event: 356

R: NO RESPONSE

NS: N12 Class: N(5.5.6.3.1) E: RESTART EQ: CR/non-zero bits 5-8. RI/Class = all channels. Event: 357

R: NO RESPONSE

NS: N10 Class: N(5.5.6.3.1) E: RESTART ACK EQ: CR/non-zero bits 5-8.

Event: 358

R: NO RESPONSE

NS: N10 Class: N(5.5.6.3.1) E: STATUS EQ: CR/non-zero bits 5-8. CS/state = U10. CA/value = 30. Event: 359

R: NO RESPONSE

NS: N10 Class: N(5.5.6.3.1) E: STATUS ENQ EQ: CR/non-zero bits 5-8.

Event: 360

R: NO RESPONSE

NS: N10 Class: N(5.5.6.3.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Call Reference non-zero bits 5-8 octet 1

B-47 ATM Forum Technical Committee

E: SETUP EQ: CR/length not equal to 3. Note 1,21.

Event: 381

R: NO RESPONSE

NS: N0 Class: N(5.5.6.3.1) E: CALL PROC EQ: CR/length not equal to 3. without CI.

Event: 382

R: NO RESPONSE

NS: N6 Class: N(5.5.6.3.1) E: CONN EQ: CR/length not equal to 3. without CI. .

Event: 383

R: NO RESPONSE

NS: N9 Class: N(5.5.6.3.1) E: CONN ACK EQ: CR/length not equal to 3. Note 16.

Event: 384

R: NO RESPONSE

NS: N10 Class: N(5.5.6.3.1) E: RELEASE EQ: CR/length not equal to 3. CA/value = 16. Event: 385

R: NO RESPONSE

NS: N10 Class: N(5.5.6.3.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Call Reference length not equal to 3

ATM Forum Technical Committee B-48

E: RELEASE COMP EQ: CR/length not equal to 3.

Event: 386

R: NO RESPONSE

NS: N12 Class: N(5.5.6.3.1) E: RESTART EQ: CR/length not equal to 3. RI/class= all channels. Event: 387

R: NO RESPONSE

NS: N10 Class: N(5.5.6.3.1) E: RESTART ACK EQ: CR/length not equal to 3. Event: 388

R: NO RESPONSE NS: N10 Class: N(5.5.6.3.1)

E: STATUS EQ: CR/length not equal to 3. CS/state = U10. CA/value = 30. Event: 389

R: NO RESPONSE

NS: N10 Class: N(5.5.6.3.1) E: STATUS ENQ EQ: CR/length not equal to 3.

Event: 390

R: NO RESPONSE

NS: N10 Class: N(5.5.6.3.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Call Reference length not equal to 3

B-49 ATM Forum Technical Committee

E: CALL PROC EQ: CR/value not in use. without CI.

Event: 411

R: RELEASE COMP RQ: CA/value = 81. NS: N0 Class: N(5.5.6.3.2 a) E: CONN EQ: CR/value not in use. without CI.

Event: 412

R: RELEASE COMP RQ: CA/value = 81. NS: N0 Class: N(5.5.6.3.2 a) E: CONN ACK EQ: CR/value not in use.

Event: 413

R: RELEASE COMP RQ: CA/value = 81. NS: N0 Class: N(5.5.6.3.2 a) E: RELEASE EQ: CR/value not in use. CA/value = 16.

Event: 414

R: RELEASE COMP RQ: CA/value = 81. NS: N0 Class: N(5.5.6.3.2 a) E: RELEASE COMP EQ: CR/value not in use.

Event: 415

R: NO RESPONSE

NS: N0 Class: N(5.5.6.3.2 b)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Call Reference value not in use

ATM Forum Technical Committee B-50

E: SETUP EQ: CR/ flag = 1. Note 1,21.

Event: 441

R: NO RESPONSE

NS: N0 Class: N(5.5.6.3.2 c) E: SETUP EQ: CR/value in use. Note 1,2,21.

Event: 442

R: NO RESPONSE

NS: N1 Class: N(5.5.6.3.2 d) E: SETUP EQ: CR/value in use. Note 1,3,21.

Event: 442

R: NO RESPONSE

NS: N3 Class: N(5.5.6.3.2 d) E: SETUP EQ: CR/value in use. Note 1,21.

Event: 443

R: NO RESPONSE

NS: N10 Class: N(5.5.6.3.2 d)

R: NO RESPONSE

NS: N12 Class: N(5.5.6.3.2 d)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Call Reference flag incorrectly set to 1 or call reference value in use

B-51 ATM Forum Technical Committee

E: SETUP

EQ: CR/global value. Note 1,21.

Event: 461

R: STATUS

RQ: CA/value = 81, CR/global value, CS/ state = Rest 0. NS: N0 Class: N(5.5.6.3.2 e)

E: CALL PROC

EQ: CR/global value. without CI.

Event: 462

R: STATUS

RQ: CA/value = 81, CR/global value, CS/ state = Rest 0. NS: N6 Class: N(5.5.6.3.2 e)

E: CONN

EQ: CR/global value. without CI.

Event: 463

R: STATUS

RQ: CA/value = 81, CR/global value, CS/ state = Rest 0. NS: N9 Class: N(5.5.6.3.2 e)

E: CONN ACK

EQ: CR/global value. Note 16.

Event: 464

R: STATUS

RQ: CA/value = 81, CR/global value, CS/ state = Rest 0. NS: N10 Class: N(5.5.6.3.2 e)

E: RELEASE

EQ: CR/global value. CA/value = 16.

Event: 465

R: STATUS

RQ: CA/value = 81, CR/global value, CS/ state = Rest 0. NS: N10 Class: N(5.5.6.3.2 e)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Call Reference global call reference

ATM Forum Technical Committee B-52

E: RELEASE COMP

EQ: CR/global value.

Event: 466

R: STATUS

RQ: CA/value = 81, CR/global value, CS/ state = Rest 0. NS: N12 Class: N(5.5.6.3.2 e)

E: STATUS ENQ

EQ: CR/global value.

Event: 467

R: STATUS

RQ: CA/value = 81, CR/global value, CS/ state = Rest 0. NS: N10 Class: N(5.5.6.3.2 e)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Call Reference global call reference

B-53 ATM Forum Technical Committee

E: CALL PROC

EQ: without CI. Note 2. Event: 501

R: STATUS RQ: CA/value = 101, 97.CS/state=N1. NS: N1 Class: I(5.5.6.4)

E: CALL PROC

EQ: without CI. Note 3. Event: 501

R: STATUS RQ: CA/value = 101, 97.CS/state=N3 NS: N3 Class: I(5.5.6.4) E: CALL PROC

EQ: without CI.

Event: 502

R: STATUS RQ: CA/value = 101, 97.CS/state=N9. NS: N9 Class: I(5.5.6.4)

R: STATUS RQ: CA/value = 101, 97.CS/state=N10. NS: N10 Class: I(5.5.6.4)

R: STATUS RQ: CA/value = 101, 97.CS/state=N12. NS: N12 Class: I(5.5.6.4) E: CONN

EQ: without CI. Note 2. Event: 503

R: STATUS RQ: CA/value = 101, 97.CS/state=N1. NS: N1 Class: I(5.5.6.4) E: CONN

EQ: without CI. Note 3. Event: 503

R: STATUS RQ: CA/value = 101, 97.CS/state=N3. NS: N3 Class: I(5.5.6.4)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Message Sequence

ATM Forum Technical Committee B-54

E: CONN

EQ: without CI.

Event: 504

R: STATUS RQ: CA/value = 101, 97.CS/state=N10. NS: N10 Class: I(5.5.6.4)

R: STATUS RQ: CA/value = 101, 97.CS/state=N12. NS: N12 Class: I(5.5.6.4) E: CONN ACK

EQ: Note 2.

Event: 505

R: STATUS RQ: CA/value = 101, 97.CS/state=N1. NS: N1 Class: I(5.5.6.4) E: CONN ACK

EQ: Note 3.

Event: 505

R: STATUS RQ: CA/value = 101, 97.CS/state=N3. NS: N1 Class: I(5.5.6.4) E: CONN ACK

Event: 506

R: STATUS RQ: CA/value = 101, 97.CS/state=N6. NS: N6 Class: I(5.5.6.4)

R: STATUS RQ: CA/value = 101, 97.CS/state=N9. NS: N9 Class: I(5.5.6.4)

R: STATUS RQ: CA/value = 101, 97.CS/state=N12. NS: N12 Class: I(5.5.6.4) E: RELEASE

EQ: CA/value = 16.

Event: 507

R: RELEASE COMP stop T303N

NS: N0 Class: I(5.5.6.4)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Message Sequence

B-55 ATM Forum Technical Committee

E: remote RELEASE EQ: without CA. Note 2. Event: 508

R: RELEASE COMP RQ: CA/value = 31. NS: N0

Class: I(5.5.6.4) E: remote RELEASE

EQ: without CA. Note 3. Event: 508

R: RELEASE start T308N RQ: CA/value = 31. NS: N12 Class: I(5.5.6.4)

E: remote RELEASE

EQ: CA/value = 41. Note 2. Event: 509

R: RELEASE COMP RQ: CA/value = 41. NS: N0 Class: I(5.5.6.4)

E: remote RELEASE EQ: CA/value = 41. Note 3.

Event: 509

R: RELEASE start T308N RQ: CA/value = 41. NS: N12 Class: I(5.5.6.4)

E: RELEASE COMP

EQ: without CA. Note 2. Event: 510

R: NO RESPONSE

NS: N0 Class: I(5.5.6.4)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Message Sequence

ATM Forum Technical Committee B-56

E: RELEASE COMP

EQ: without CA. Note 3. Event: 510

R: NO RESPONSE

NS: N0 Class: I(5.5.6.4) E: RELEASE COMP

EQ: without CA.

Event: 511

R: NO RESPONSE

NS: N0 Class: I(5.5.6.4)

R: NO RESPONSE

NS: N0 Class: I(5.5.6.4) E: remote RELEASE COMP

EQ: without CA.

Event: 512

R: RELEASE start T308N RQ: CA/value = 111.

NS: N12 Class: I(5.5.6.4) E: remote RELEASE COMP

EQ: CA/value = 41.

Event: 513

R: RELEASE start T308N RQ: CA/value = 41.

NS: N12 Class: I(5.5.6.4) E: UNRECOGNIZED

EQ: Note 2.

Event: 514

R: STATUS RQ: CA/value = 97, 101. CS/state=N1.

NS: N1 Class: N(5.5.6.4)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Message Sequence

B-57 ATM Forum Technical Committee

E: UNRECOGNIZED

EQ: Note 3.

Event: 514

R: STATUS RQ: CA/value = 97, 101. CS/state= N3.

NS: N3 Class: N(5.5.6.4) E: UNRECOGNIZED

Event: 515

R: STATUS RQ: CA/value = 97, 101. CS/state=N6.

NS: N6 Class: N(5.5.6.4)

R: STATUS RQ: CA/value = 97, 101. CS/state=N9.

NS: N9 Class: N(5.5.6.4)

R: STATUS RQ: CA/value = 97, 101. CS/state=N10

NS: N10 Class: N(5.5.6.4)

R: STATUS RQ: CA/value = 97, 101. CSstate=N12.

NS: N12 Class: N(5.5.6.4) E: ALERTING (IUT-T)

EQ: Note 2.

Event: 516

R: STATUS RQ: CA/value = 97, 101.CS/state=N1.

NS: N1 Class: N(5.5.6.4) E: ALERTING (IUT-T)

EQ: Note 3.

Event: 516

R: STATUS RQ: CA/value = 97, 101. CS/state=N3.

NS: N3 Class: N(5.5.6.4) E: ALERTING (IUT-T)

Event: 517

R: STATUS RQ: CA/value = 97, 101. CS/state=N6.

NS: N6 Class: N(5.5.6.4)

R: STATUS RQ: CA/value = 97, 101. CS/state=N9.

NS: N9 Class: N(5.5.6.4)

R: STATUS RQ: CA/value = 97, 101.CS/state=N10.

NS: N10 Class: N(5.5.6.4)

R: STATUS RQ: CA/value = 97, 101.CS/state=N12.

NS: N12 Class: N(5.5.6.4)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Message Sequence

ATM Forum Technical Committee B-58

E: SETUP EQ: mandatory missing (ATD). Note 1,21. Event: 551

R: RELEASE COMP RQ: CA/value = 96. NS: N0 Class: N(5.5.6.7.1) E: SETUP EQ: mandatory missing (BBC). Note 1,21.

Event: 552

R: RELEASE COMP RQ: CA/value = 96. NS: N0 Class: N(5.5.6.7.1) E: SETUP EQ: mandatory missing (CDN). Note 1,21.

Event: 553

R: RELEASE COMP RQ: CA/value = 96. NS: N0 Class: N(5.5.6.7.1) E: SETUP EQ: mandatory missing (QOS). Note 1,21. Event: 554

R: RELEASE COMP RQ: CA/value = 96. NS: N0 Class: N(5.5.6.7.1) E: RELEASE EQ: mandatory missing (CA).

Event: 555

R: RELEASE COMP RQ: CA/value = 96. NS: N0 Class: N(5.5.6.7.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Mandatory mandatory IE. missing

B-59 ATM Forum Technical Committee

E: RELEASE COMP

EQ: mandatory missing (CA).

Event: 556

R: NO RESPONSE stop T303N

NS: N0 Class: N(5.5.6.7.1)

E: RESTART

EQ: mandatory missing (RI).without CI.

Event: 557

R: STATUS

RQ: CA/value = 96. CR/ global value. CS/ state= Rest0 NS: N10 Class: N(5.5.6.7.1)

E: RESTART

EQ: mandatory missing (CI). RI/class = indicated channel.

Event: 558

R: STATUS

RQ: CA/value = 96. CR/global value. CS/ state=Rest0. NS: N10 Class: N(5.5.5.2)

E: STATUS

EQ: mandatory missing (CS).CA/value = 30. Event: 559

R: STATUS

RQ: CA/value = 96. CS/state =N10

NS: N10 Class: N(5.5.6.7.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Mandatory mandatory IE. missing

ATM Forum Technical Committee B-60

E: SETUP

EQ:mandatory invalid content (length of ATD= 31). Note 1,21. Event: 601

R: RELEASE COMP RQ: CA/value = 100.

NS: N0 Class: N(5.5.6.7.2) E: SETUP EQ:mandatory invalid content (ATD/coding standard = 01B). Note 1,21. Event: 602

R: RELEASE COMP RQ: CA/value = 100.

NS: N0 Class: N(5.5.6.6.3) E: SETUP EQ:mandatory invalid content (ATD/ PCR(CLP=0+1) identifier. Note 1,21. Event: 603

R: RELEASE COMP RQ: CA/value = 100.

NS: N0 Class: N(5.5.6.7.2) E: SETUP

EQ:mandatory invalid content (length of BBC = 8). Note 1,21. Event: 604

R: RELEASE COMP RQ: CA/value = 100.

NS: N0 Class: N(5.5.6.7.2) E: SETUP EQ:mandatory invalid content (BBC/coding standard = 01B). Note 1, 21. Event: 605

R: RELEASE COMP RQ: CA/value = 100.

NS: N0 Class: N(5.5.6.7.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Mandatory mandatory IE. invalid content

B-61 ATM Forum Technical Committee

E: SETUP EQ:mandatory invalid content (BBC/bearer class = 11111B). Note 1,21. Event: 606

R: RELEASE COMP RQ: CA/value = 100.

NS: N0

Class: N(5.5.6.7.2) E: SETUP EQ:mandatory invalid content (BBC/traffic type = 111B). (BBC Class =X. Note 1,21. Event: 607

R: RELEASE COMP RQ: CA/value = 100.

NS: N0

Class: N(5.5.6.7.2) E: SETUP EQ:mandatory invalid content (BBC/user plane connection configuration = 11B). Note 1,21. Event: 608

R: RELEASE COMP RQ: CA/value = 100.

NS: N0

Class: N(5.5.6.7.2) E: SETUP EQ:mandatory invalid content (BBC/spare (octet 6) = 111B). Note 1,2,21. Event: 609

R: NO RESPONSE

NS: N1.

Class: I(5.4.5.1) E: SETUP EQ:mandatory invalid content (BBC/spare (octet 6) = 111B). Note 1,3,21. Event: 609

R: CALL PROC RQ: with a valid CI.

NS: N3.

Class: I(5.4.5.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Mandatory mandatory IE. invalid content

ATM Forum Technical Committee B-62

E: SETUP

EQ:mandatory invalid content (CDN exceed the maximum length). Note 1,21. Event: 610

R: RELEASE COMP RQ: CA/value = 100.

NS: N0

Class: N(5.5.6.7.2) E: SETUP EQ:mandatory invalid content (CDN/coding standard = 01B). Note 1,21. Event: 611

R: RELEASE COMP RQ: CA/value = 100.

NS: N0

Class: N(5.5.6.7.2) E: SETUP EQ:mandatory invalid content (CDN/type of number = 111B). Note 1,21. Event: 612

R: RELEASE COMP RQ: CA/value = 100.

NS: N0

Class: N(5.5.6.7.2) E: SETUP EQ:mandatory invalid content (CDN/numbering plan= 1111B). Note 1,21. Event: 613

R: RELEASE COMP RQ: CA/value = 100.

NS: N0

Class: N(5.5.6.7.2) E: SETUP EQ:mandatory invalid content (CDN/Invalid number. Note 1,2,5,21.

Event: 614

R: RELEASE COMP

RQ: CA/value = 1,3,22, 28. NS: N0 Class: N(5.5.1.4)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Mandatory mandatory IE. invalid content

B-63 ATM Forum Technical Committee

E: SETUP EQ:mandatory invalid content (CDN/Invalid number. Note 1,3,5,21.

Event: 614

R: CALL PROC + RELEASE start T308N RQ: CA/value = 1,3,22, 28. NS: N12 Class: N(5.5.1.4)

E: SETUP EQ:mandatory invalid content (length of QOS = 7).Note 1,21. Event: 615

R: RELEASE COMP RQ: CA/value = 100.

NS: N0

Class: N(5.5.6.7.2) E: SETUP EQ:mandatory invalid content (QOS/coding standard= 01B). Note 1,21. Event: 616

R: RELEASE COMP RQ: CA/value = 100.

NS: N0

Class: N(5.5.6.7.2 E: SETUP EQ:mandatory invalid content (QOS/qos class F. = 11110000B). Note 1,21. Event: 617

R: RELEASE COMP RQ: CA/value = 100.

NS: N0

Class: N(5.5.6.7.2) E: SETUP EQ:mandatory invalid content (QOS/qos class B. = 11110000B). Note 1,21. Event: 618

R: RELEASE COMP RQ: CA/value = 100.

NS: N0

Class: N(5.5.6.7.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Mandatory mandatory IE. invalid content

ATM Forum Technical Committee B-64

E: CALL PROC

EQ:mandatory invalid content (length of CI = 10).

Event: 619

R: STATUS

RQ: CA/value = 100. CS/state=N6.

NS: N6 Class: N(5.5.6.7.2)

E: CALL PROC

EQ: non-mandatory invalid content (length of CI = 10).

Event: 619

R: NO RESPONSE or STATUS RQ: CA/value = 100. CS/state=N9.

NS: N9 Class: N(5.5.6.8.2) E: CALL PROC

EQ:mandatory invalid content (CI/vp associated signalling = 11B).

Event: 620

R: STATUS

RQ: CA/value = 100. CS/state=N6.

NS: N6 Class: N(5.5.6.7.2)

E: CALL PROC EQ: non-mandatory invalid content (CI/vp associated signalling = 11B).

Event: 620

R: NO RESPONSE or STATUS RQ: CA/value = 100. CS/state=N9.

NS: N9 Class: N(5.5.6.8.2) E: CALL PROC

EQ:mandatory invalid content (CI/prefered exclusive = 111B).

Event: 621

R: STATUS

RQ: CA/value = 100. CS/state=N6.

NS: N6 Class: N(5.5.6.7.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Mandatory mandatory IE. invalid content

B-65 ATM Forum Technical Committee

E: CALL PROC EQ: non-mandatory invalid content (CI/ prefered exclusive = 111B).

Event: 621

R: NO RESPONSE or STATUS RQ: CA/value = 100. CS/state=N9.

NS: N9 Class: N(5.5.6.8.2) E: CALL PROC

EQ:mandatory invalid content (CI/vci = 10, vpci= any valid).

Event: 622

R: RELEASE stop T303N start T308N

RQ: CA/value = 36.

NS: N12 Class: N(5.5.2.3)

E: CALL PROC EQ: non-mandatory invalid content (CI/vci = 10, vpci= any valid).

Event: 622

R: NO RESPONSE or STATUS RQ: CA/value = 100. CS/state=N9.

NS: N9 Class: N(5.5.6.7.2) E: CALL PROC

EQ:mandatory invalid content (CI/vpci = 300, vci= any valid).

Event: 623

R: RELEASE stop T303N start T308N

RQ: CA/value = 36.

NS: N12 Class: N(5.5.2.3)

E: CALL PROC

EQ: non-mandatory invalid content (CI/vpci = 300, vci= any valid).

Event: 623

R: NO RESPONSE or STATUS RQ: CA/value = 100. CS/state=N9.

NS: N9 Class: N(5.5.6.7.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Mandatory mandatory IE. invalid content

ATM Forum Technical Committee B-66

E: CALL PROC

EQ:mandatory invalid content (CI/spare = 11B).

Event: 624

R: NO RESPONSE stop T303N, start T310N

NS: N9

Class: I(5.4.5.1) E: CONN

EQ:mandatory invalid content (CI/coding standard = 01B).

Event: 625

R: STATUS

RQ: CA/value = 100. CS/state=N6.

NS: N6 Class: N(5.5.6.7.2)

E: CONN

EQ: non-mandatory invalid content (CI/coding standard = 01B).

Event: 625

R: CONN ACK or CONN ACK +STA- TUS RQ: CA/value = 100. CS/state=N10. NS: N10 Class: N(5.5.6.8.2) E: CONN

EQ:mandatory invalid content (CI/vci = 20, vpci= any valid).

Event: 626

R: RELEASE stop T303N start T308N

RQ: CA/value = 36..

NS: N12 Class: N(5.5.2.3)

E: CONN

EQ: non-mandatory invalid content (CI/vci = 20, vpci= any valid).

Event: 626

R: CONN ACK or CONN ACK + STA- TUS RQ: CA/value = 100. CS/state=N10. NS: N10 Class: N(5.5.6.8.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Mandatory mandatory IE. invalid content.

B-67 ATM Forum Technical Committee

E: CONN EQ:mandatory invalid content (CI/vpci = 0, vci= 5 signalling). Event: 627

R: RELEASE stop T303N start T308N RQ: CA/value = 36.

NS: N12 Class: N(5.5.2.3) E: CONN EQ: non-mandatory invalid content (CI/vpci = 0, vci= 5 signalling). Event: 627

R: CONN ACK or CONN ACK + STA- TUS RQ: CA/value = 100. CS/state=N10. NS: N10 Class: N(5.5.6.8.2) E: CONN

EQ:mandatory invalid content (CI/spare = 11B). Note 1. Event: 628

R: CONN ACK stop T303N

NS: N10 Class: I(5.4.5.1) E: RELEASE

EQ:mandatory invalid content (length of CA= 35). Event: 629

R: RELEASE COMP RQ: CA/value = 100.

NS: N0

Class: N(5.5.6.7.2) E: RELEASE

EQ:mandatory invalid content (CA/location = 1111B). Event: 630

R: RELEASE COMP RQ: CA/value = 100.

NS: N0

Class: N(5.5.6.7.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Mandatory mandatory IE. invalid content

ATM Forum Technical Committee B-68

E: RELEASE EQ:mandatory invalid content (CA/value = 0).

Event: 631

R: RELEASE COMP RQ: CA/value = 100. NS: N0 Class: N(5.5.6.7.2) E: RELEASE EQ:mandatory invalid content (CA/spare = 111B). Event: 632

R: RELEASE COMP

NS: N0

Class: I(5.4.5.1) E: RELEASE COMP EQ:mandatory invalid content (CA/location = 1111B). Event: 633

R: NO RESPONSE stop T303N NS: N0 Class: N(5.5.6.7.2) E: RELEASE COMP

EQ:mandatory invalid content (CA/value=0). Event: 634

R: NO RESPONSE stop T303N NS: N0 Class: N(5.5.6.7.2) E: RELEASE COMP EQ:mandatory invalid content (CA/spare = 111B). Event: 635

R: NO RESPONSE stop T303N NS: N0 Class: I(5.4.5.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Mandatory mandatory IE. invalid content

B-69 ATM Forum Technical Committee

E: RESTART

EQ:mandatory invalid content (length of RI = 6). Event: 636

R: STATUS

RQ: CR/global value. CA/value = 100. CS/ state=Rest 0. NS: N10 Class: N(5.5.6.7.2)

E: RESTART

EQ:mandatory invalid content (RI/coding standard = 01B).

Event: 637

R: STATUS

RQ: CR/global value. CA/value = 100. CS/ state=Rest 0. NS: N10 Class: N(5.5.6.7.2)

E: RESTART

EQ:mandatory invalid content (RI/class = 111B).

Event: 638

R: STATUS

RQ: CR/global value. CA/value = 100. CS/ state=Rest 0. NS: N10 Class: N(5.5.6.7.2)

E: RESTART EQ:mandatory invalid content (RI/class= indicated channel, CI/vpci=0,vci=5 (reserved for signalling)). Event: 639

R: STATUS

RQ: CR/global value. CA/value = 82. CS/ state= Rest 0. NS: N10 Class: N(5.5.5.2)

E: RESTART

EQ:mandatory invalid content (RI/spare = 1111B).

Event: 640

R: RESTART ACK

NS: N0

Class: I(5.4.5.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Mandatory mandatory IE. invalid content

ATM Forum Technical Committee B-70

E: STATUS

EQ:mandatory invalid content (CS/state = 111111B). Event: 641

R: STATUS RQ: CA/value = 100. CS/state = N10. NS: N10

Class: N(5.5.6.7.2) E: STATUS

EQ:mandatory invalid content (length of CS = 6). Event: 642

R: STATUS RQ: CA/value = 100. CS/state = N10. NS: N10

Class: N(5.5.6.7.2) E: STATUS EQ:mandatory invalid content (CS/spare = 11B, state = U10, CA/ value = 30). Event: 643

R: NO RESPONSE

NS: N10

Class: I(5.4.5.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Mandatory mandatory IE. invalid content.

B-71 ATM Forum Technical Committee

E: SETUP

EQ: unrecognized IE. Note 1,2,5,21,31.

Event: 701

R: NO RESPONSE

NS: N1

Class: I(5.5.6.8.1) E: SETUP

EQ: unrecognized IE. Note 1,3,5,21,31.

Event: 701

R: CALL PROC

RQ: with a valid CI.

NS: N3 Class: I(5.5.6.8.1) E: SETUP

EQ: unrecognized IE. Note 1,2,5,21,32,.

Event: 701

R: STATUS RQ: CA/value = 99, CS/state = N1. NS: N1

Class: I(5.5.6.8.1)

E: SETUP

EQ: unrecognized IE. Note 1,3,5,21,32.

Event: 701

R: CALL PROC + STATUS RQ: with a valid CI. CA/value = 99, CS/state = N3. NS: N3 Class: I(5.5.6.8.1) E: SETUP

EQ: unrecognized IE (BLSH). Note 1,2,5,21,31. Event: 702

R: NO RESPONSE

NS: N1

Class: I(5.4.5.3)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory unrecognized IE.

ATM Forum Technical Committee B-72

E: SETUP

EQ: unrecognized IE (BLSH). Note 1,3,5,21,31. Event: 702

R: CALL PROC

RQ: with a valid CI.

NS: N3 Class: I(5.4.5.3) E: SETUP

EQ: unrecognized IE (BLSH). Note 1,2,5,21,32. Event: 702

R: STATUS RQ: CA/value = 99, CS/state = N1.

NS: N1 Class: I(5.4.5.3) E: SETUP

EQ: unrecognized IE (BLSH). Note 1,3,5,21,32. Event: 702

R: CALL PROC + STATUS RQ: with a valid CI. CA/value = 99, CS/state = N3. NS: N3 Class: I(5.4.5.3) E: SETUP

EQ: unrecognized IE (BNSH). Note 1,2,5,21,31. Event: 703

R: NO RESPONSE

NS: N1

Class: I(5.4.5.4) E: SETUP

EQ: unrecognized IE (BNSH). Note 1,3,5,21,31. Event: 703

R: CALL PROC

RQ: with a valid CI.

NS: N3 Class: I(5.4.5.4)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory unrecognized IE.

B-73 ATM Forum Technical Committee

E: SETUP

EQ: unrecognized IE (BNSH). Note 1,2,5,21,32.

Event: 703

R: STATUS RQ: CA/value = 99, CS/state = N1.

NS: N1

Class: I(5.4.5.4)

E: SETUP

EQ: unrecognized IE (BNSH). Note 1,3,5,21,32.

Event: 703

R: CALL PROC + STATUS RQ: with a valid CI. CA/value = 99, CS/state = N3. NS: N3 Class: I(5.4.5.4) E: remote SETUP

EQ: unrecognized IE. Note 1,21.

Event: 704

R: SETUP start T303N RQ: with CI and without unregonized IE. Note 17,18. NS: N6 Class: I(5.5.6.8.1) E: remote SETUP

EQ: unrecognized IE. (BLSH). Note 1,21.

Event: 705

R: SETUP start T303N RQ: with a valid CI and without BLSH. Note 17,18. NS: N6 Class: I(5.5.6.8.1) E: remote SETUP

EQ: unrecognized IE. (BNSH). Note 1,21.

Event: 706

R: SETUP start T303N RQ: with a valid CI and without BNSH. Note 17,18. NS: N6 Class: I(5.5.6.8.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix

Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory unrecognized IE.

ATM Forum Technical Committee B-74

E: CALL PROC

EQ: unrecognized IE. without CI. Note 31.

Event: 707

R: NO RESPONSE stop T303N, start T310N

NS: N9 Class: I(5.5.6.8.1) E: CALL PROC

EQ: unrecognized IE. without CI. Note 32.

Event: 707

R: STATUS stop T303N, start T310N RQ: CA/value = 99, CS/state = N9. NS: N9 Class: I(5.5.6.8.1) E: CONN

EQ: unrecognized IE. without CI. Note 31.

Event: 708

R: CONN ACK stop T310N

NS: N10 Class: I(5.5.6.8.1) E: CONN

EQ: unrecognized IE. without CI. Note 32.

Event: 708

R: CONN ACK + STATUS stop T310N RQ: CA/value = 99, CS/state = N10. NS: N10 Class: I(5.5.6.8.1) E: remote CONN

EQ: unrecognized IE. Note 3.

Event: 709

R: CONN

RQ: without unrecognized IE. NS: N10

Class: I(5.5.6.8.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory unrecognized IE.

B-75 ATM Forum Technical Committee

E: remote CONN EQ: unrecognized IE. Note 2.

Event: 709

R: CONN RQ: with CI and without unrecognized IE. NS: N10 Class: I(5.5.6.8.1) E: remote CONN EQ: unrecognized IE (BLSH). Note 3.

Event: 710

R: CONN

RQ: without BLSH. NS: N10 Class: I(5.4.5.3) E: remote CONN EQ: unrecognized IE. (BLSH) Note 2.

Event: 710

R: CONN RQ: with CI and without BLSH. NS: N10 Class: I(5.4.5.3) E: remote CONN EQ: unrecognized IE (BNSH). Note 3.

Event: 711

R: CONN RQ: without BNSH. NS: N10 Class: I(5.4.5.4) E: remote CONN EQ: unrecognized IE. (BNSH). Note 2.

Event: 711

R: CONN RQ: with CI and without BNSH. NS: N10 Class: I(5.4.5.4)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory unrecognized IE

ATM Forum Technical Committee B-76

E: CONN ACK

EQ: unrecognized IE. Note 16,31.

Event: 712

R: NO RESPONSE

NS: N10 Class: I(5.5.6.8.1) E: CONN ACK

EQ: unrecognized IE. Note 16,32.

Event: 712

R: STATUS

RQ: CA/value = 99, CS/state =N10. NS: N10 Class: I(5.5.6.8.1) E: RELEASE

EQ: unrecognized IE.CA/value = 16.

Event: 713

R: RELEASE COMP RQ: CA/value = 99.

NS: N0 Class: I(5.5.6.8.1) E: RELEASE COMP

EQ: unrecognized IE.

Event: 714

R: NO RESPONSE stop T308N

NS: N0 Class: I(5.5.6.8.1) E: RESTART

EQ: unrecognized IE.RI/Class = all channels. Note 31. Event: 715

R: RESTART ACK

NS: N0 Class: I(5.5.6.8.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory unrecognized IE.

B-77 ATM Forum Technical Committee

E: RESTART

EQ: unrecognized IE.RI/Class = all channels. Note 32.

Event: 715

R: RESTART ACK + STATUS RQ: CR/global value. CA/value = 99, CS/state = Rest0. NS: N0 Class: I(5.5.6.8.1) E: STATUS

EQ: unrecognized IE. CS/state = U10, CA/ value = 30. Note 31.

Event: 716

R: NO RESPONSE

NS: N10

Class: I(5.5.6.8.1)

E: STATUS

EQ: unrecognized IE. CS/state = U10, CA/ value = 30. Note 32.

Event: 716

R: STATUS RQ: CA/value = 99, CS/state = N10. NS: N10

Class: I(5.5.6.8.1)

E: STATUS ENQ

EQ: unrecognized IE.

Event: 717

R: STATUS

RQ:CA/value = 30,99, CS/state = N10. NS: N10

Class: I(5.5.6.8.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory IE. unrecognized IE.

ATM Forum Technical Committee B-78

E: SETUP EQ: non-mandatory error (AALP/coding standard = 01B). Note 2,5, 21,31.

Event: 731

R: NO RESPONSE

NS: N1

Class: N(5.5.6.6.3)

E: SETUP EQ: non-mandatory error (AALP/coding standard = 01B). Note 3,5,21,31.

Event: 731

R: CALL PROC

RQ: with a valid CI.

NS: N3

Class: N(5.5.6.6.3) E: SETUP EQ: non-mandatory error (AALP/coding standard = 01B). Note 2,5,21,32.

Event: 731

R: STATUS RQ: CA/value = 100, CS/state = N1. NS: N1

Class: N(5.5.6.6.3)

E: SETUP EQ: non-mandatory error (AALP/coding standard = 01B). Note 3,5,21,32.

Event: 731

R: CALL PROC+ STATUS RQ: with a valid CI. CA/value = 100, CS/ state = N3. NS: N3 Class: N(5.5.6.6.3) E: SETUP

EQ: non-mandatory error (length of AALP > 21). Note 2,5,21,31.

Event: 732

R: NO RESPONSE

NS: N1

Class: N(5.5.6.8.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory IE. content error

B-79 ATM Forum Technical Committee

E: SETUP

EQ: non-mandatory error (length of AALP > 21). Note 3,5,21,31.

Event: 732

R: CALL PROC

RQ: with a valid CI.

NS: N3

Class: N(5.5.6.8.2) E: SETUP

EQ: non-mandatory error (length of AALP > 21). Note 2,5,21,32.

Event: 732

R: STATUS RQ: CA/value = 43, CS/state = N1. NS: N1

Class: N(5.5.6.8.2)

E: SETUP

EQ: non-mandatory error (length of AALP > 21). Note 3,5,21,32.

Event: 732

R: CALL PROC+ STATUS RQ: with a valid CI. CA/value = 43, CS/state = N3. NS: N3 Class: N(5.5.6.8.2) E: SETUP EQ: non-mandatory error (AALP/AAL type = 11111111B). Note 2,5,21,31.

Event: 733

R: NO RESPONSE

NS: N1

Class: N(5.5.6.8.2)

E: SETUP EQ: non-mandatory error (AALP/AAL type = 11111111B). Note 3,5,21,31.

Event: 733

R: CALL PROC

RQ: with a valid CI.

NS: N3

Class: N(5.5.6.8.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory IE. content error

ATM Forum Technical Committee B-80

E: SETUP EQ: non-mandatory error (AALP/AAL type = 11111111B). Note 2,5,21,32.

Event: 733

R: STATUS RQ: CA/value = 100, CS/state = N1. NS: N1

Class: N(5.5.6.8.2)

E: SETUP EQ: non-mandatory error (AALP/AAL type = 11111111B). Note 3,5,21,32.

Event: 733

R: CALL PROC + STATUS RQ: with a valid CI. CA/value = 100, CS/ state = N3. NS: N3 Class: N(5.5.6.8.2) E: SETUP

EQ: non-mandatory error (BHL/coding standard = 01B). Note 2,5,7,21,31. Event: 734

R: NO RESPONSE

NS: N1

Class: N(5.5.6.6.3)

E: SETUP

EQ: non-mandatory error (BHL/coding standard = 01B). Note 3,5,7,21,31. Event: 734

R: CALL PROC

RQ: with a valid CI.

NS: N3

Class: N(5.5.6.6.3) E: SETUP

EQ: non-mandatory error (BHL/coding standard = 01B). Note 2,5,7,21,32. Event: 734

R: STATUS

RQ: CA/value = 100, CS/state = N1. NS: N1

Class: N(5.5.6.6.3)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory IE. content error

B-81 ATM Forum Technical Committee

E: SETUP

EQ: non-mandatory error (BHL/coding standard = 01B). Note 3,5,7,21,32. Event: 734

R: CALL PROC + STATUS RQ: with a valid CI. CA/value = 100, CS/ state = N3. NS: N3 Class: N(5.5.6.6.3) E: SETUP

EQ: non-mandatory error (length of BHL > 14). Note 2,5,7,21,31.

Event: 735

R: NO RESPONSE

NS: N1

Class: N(5.5.6.8.2)

E: SETUP

EQ: non-mandatory error (length of BHL > 14). Note 3,5,7,21,31.

Event: 735

R: CALL PROC

RQ: with a valid CI.

NS: N3

Class: N(5.5.6.8.2) E: SETUP

EQ: non-mandatory error(length of BHL > 14). Note 2,5,7,21,32.

Event: 735

R: STATUS

RQ: CA/value = 43, CS/state = N1. NS: N1

Class: N(5.5.6.8.2)

E: SETUP

EQ: non-mandatory error (length of BHL > 14). Note 3,5,7,21,32.

Event: 735

R: CALL PROC + STATUS RQ: with a valid CI. CA/value = 43, CS/state =N3. NS: N3 Class: N(5.5.6.8.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory IE. content error

ATM Forum Technical Committee B-82

E: SETUP EQ: non-mandatory error(BHL/layer information type = 1111111 B). Note 2,5,7,21,31.

Event: 736

R: NO RESPONSE

NS: N1

Class: N(5.5.6.8.2)

E: SETUP EQ: non-mandatory error (BHL/layer information type = 1111111 B). Note 3,5,7.21,31.

Event: 736

R: CALL PROC

RQ: with a valid CI.

NS: N3

Class: N(5.5.6.8.2) E: SETUP EQ: non-mandatory error (BHL/layer information type = 1111111 B). Note 2,5,7,21,32.

Event: 736

R: STATUS

RQ: CA/value = 100, CS/state = N1. NS: N1

Class: N(5.5.6.8.2)

E: SETUP EQ: non-mandatory error (BHL/layer information type = 1111111 B). Note 3,5,7,21,32.

Event: 736

R: CALL PROC + STATUS RQ: with a valid CI. CA/value = 100, CS/ state = N3. NS: N3 Class: N(5.5.6.8.2) E: SETUP EQ: non-mandatory error (BLL/coding standard = 01B). Note 2,5,21,31.

Event: 737

R: NO RESPONSE.

NS: N1

Class: N(5.5.6.6.3)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory IE. content error

B-83 ATM Forum Technical Committee

E: SETUP EQ: non-mandatory error (BLL/coding standard = 01B). Note 3,5,21,31.

Event: 737

R: CALL PROC

RQ: with a valid CI.

NS: N3

Class: N(5.5.6.6.3) E: SETUP EQ: non-mandatory error (BLL/coding standard = 01B). Note 2,5,21,32.

Event: 737

R: STATUS

RQ: CA/value = 100, CS/state = N1.

NS: N1 Class: N(5.5.6.6.3) E: SETUP EQ: non-mandatory error (BLL/coding standard = 01B). Note 3,5,21,32.

Event: 737

R: CALL PROC + STATUS RQ: with a valid CI. CA/value = 100, CS/ state = N3. NS: N3 Class: N(5.5.6.6.3) E: SETUP

EQ: non-mandatory error (BLL/length > 18). Note 2,5,21,31.

Event: 738

R: NO RESPONSE.

NS: N1

Class: N(5.5.6.8.2)

E: SETUP

EQ: non-mandatory error (length of BLL > 18). Note 3,5,21,31.

Event: 738

R: CALL PROC

RQ: with a valid CI.

NS: N3

Class: N(5.5.6.8.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory IE. content error

ATM Forum Technical Committee B-84

E: SETUP

EQ: non-mandatory error (length of BLL > 18). Note 2,5,21,32. Event: 738

R: STATUS RQ: CA/value = 43, CS/state = N1. NS: N1

Class: N(5.5.6.8.2) E: SETUP

EQ: non-mandatory error (length of BLL > 18). Note 3,5,21,32. Event: 738

R: CALL PROC + STATUS RQ: with a valid CI. CA/value = 43, CS/state = N3. NS: N3 Class: N(5.5.6.8.2) E: SETUP

EQ: non-mandatory error (length of CDS > 25). Note 2,5,21,30,31. Event: 739

R: NO RESPONSE

NS: N1

Class: N(5.5.6.8.2) E: SETUP

EQ: non-mandatory error (length of CDS > 25). Note 3,5,21,30,31. Event: 739

R: CALL PROC

RQ: with a valid CI. NS: N3

Class: N(5.5.6.8.2) E: SETUP

EQ: non-mandatory error (length of CDS > 25). Note 2,5,21,30,32. Event: 739

R: STATUS RQ: CA/value = 43, CS/state = N1. NS: N1

Class: N(5.5.6.8.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory IE. content error

B-85 ATM Forum Technical Committee

E: SETUP

EQ: non-mandatory error (length of CDS > 25). Note 3,5,21,30,32.

Event: 739

R: CALL PROC + STATUS RQ: with a valid CI. CA/value = 43, CS/state = N3. NS: N3 Class: N(5.5.6.8.2) E: SETUP EQ: non-mandatory error (CDS/type of subaddress = 111B). Note 2,5,21,30,31.

Event: 740

R: NO RESPONSE

NS: N1

Class: N(5.5.6.8.2)

E: SETUP EQ: non-mandatory error (CDS/type of subaddress = 111B). Note 3,5,21,30,31.

Event: 740

R: CALL PROC

RQ: with a valid CI.

NS: N3

Class: N(5.5.6.8.2) E: SETUP EQ: non-mandatory error (CDS/type of subaddress = 111B). Note 2,5,21,30,32.

Event: 740

R: STATUS RQ: CA/value = 100, CS/state = N1.

NS: N1

Class: N(5.5.6.8.2)

E: SETUP EQ: non-mandatory error (CDS/type of subaddress = 111B). Note 3,5,21,30,32.

Event: 740

R: CALL PROC + STATUS RQ: with a valid CI. CA/value = 100, CS/ state = N3. NS: N3 Class: N(5.5.6.8.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory IE. content error

ATM Forum Technical Committee B-86

E: SETUP EQ: non-mandatory error (CDS/spare = 111B). Note 2,5,21,30. Event: 741

R: NO RESPONSE NS: N1

Class: I(5.4.5.1)

E: SETUP

EQ: non-mandatory error (CDS/spare = 111B). Note 3,5,21,30. Event: 741

R: CALL PROC

RQ: with a valid CI. NS: N3

Class: I(5.4.5.1) E: SETUP EQ: non-mandatory error (CGS/type of subaddress = 111B). Note 2,5,21,30,31. Event: 742

R: NO RESPONSE

NS: N1

Class: N(5.5.6.8.2) E: SETUP EQ: non-mandatory error (CGS/type of subaddress = 111B). Note 3,5,21,30,31. Event: 742

R: CALL PROC

RQ: with a valid CI. NS: N3

Class: N(5.5.6.8.2) E: SETUP EQ: non-mandatory error (CGS/type of subaddress = 111B). Note 2,5,21,30,32. Event: 742

R: STATUS RQ: CA/value = 100, CS/state = N1. NS: N1

Class: N(5.5.6.8.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory IE. content error

B-87 ATM Forum Technical Committee

E: SETUP EQ: non-mandatory error (CGS/type of subaddress = 111B). Note 3,5,21,30,32.

Event: 742

R: CALL PROC + STATUS RQ: with a valid CI. CA/value = 100, CS/ state = N3. NS: N3 Class: N(5.5.6.8.2) E: SETUP

EQ: non-mandatory error (CGS/spare = 111B). Note 2,5,21,30.

Event: 743

R: NO RESPONSE

NS: N1

Class: I(5.4.5.1)

E: SETUP

EQ: non-mandatory error (CGS/spare = 111B). Note 3,5,21,30.

Event: 743

R: CALL PROC

RQ: with a valid CI.

NS: N3

Class: I(5.4.5.1) E: SETUP EQ: non-mandatory error (CGN/type of number = 111B). Note 2,5,31.

Event: 744

R: NO RESPONSE

NS: N1

Class: N(5.5.6.8.2) E: SETUP EQ: non-mandatory error (CGN/type of number = 111B). Note 3,5,31.

Event: 744

R: CALL PROC

RQ: with a valid CI.

NS: N3

Class: N(5.5.6.8.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory IE. content error

ATM Forum Technical Committee B-88

E: SETUP EQ: non-mandatory error (CGN/type of number = 111B). Note 2,5,32.

Event: 744

R: STATUS RQ: CA/value = 100, CS/state = N1.

NS: N1

Class: N(5.5.6.8.2)

E: SETUP EQ: non-mandatory error (CGN/type of number = 111B). Note 3,5,32.

Event: 744

R: CALL PROC + STATUS RQ: with a valid CI. CA/value = 100, CS/ state = N3. NS: N3 Class: N(5.5.6.8.2) E: SETUP EQ: non-mandatory error (CGN/numbering plan = 1111B). Note 2,5,31.

Event: 745

R: NO RESPONSE

NS: N1

Class: N(5.5.6.8.2)

E: SETUP EQ: non-mandatory error (CGN/numbering plan = 1111B). Note 1, 3,5,31.

Event: 745

R: CALL PROC

RQ: with a valid CI.

NS: N3

Class: N(5.5.6.8.2) E: SETUP EQ: non-mandatory error (CGN/numbering plan = 1111B). Note 2,5,32.

Event: 745

R: STATUS RQ: CA/value = 100, CS/state = N1.

NS: N1

Class: N(5.5.6.8.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory IE. content error

B-89 ATM Forum Technical Committee

E: SETUP EQ: non-mandatory error (CGN/numbering plan = 1111B). Note 3,5,32.

Event: 745

R: CALL PROC + STATUS RQ: with a valid CI. CA/value = 100, CS/ state = N3. NS: N3 Class: N(5.5.6.8.2) E: SETUP EQ: non-mandatory error (CGN/invalid number). Note 2,5,31.

Event: 746

R: NO RESPONSE

NS: N1

Class: N(5.5.6.8.2)

E: SETUP EQ: non-mandatory error (CGN/invalid Number). Note 3,5,31.

Event: 746

R: CALL PROC

RQ: with a valid CI.

NS: N3

Class: N(5.5.6.8.2) E: SETUP EQ: non-mandatory error (CGN/invalid number). Note 2,5,32.

Event: 746

R: STATUS RQ: CA/value = 100, CS/state = N1.

NS: N1 Class: N(5.5.6.8.2)

E: SETUP EQ: non-mandatory error (CGN/invalid number). Note 3,5,32.

Event: 746

R: CALL PROC + STATUS RQ: with a valid CI. CA/value = 100, CS/ state = N3. NS: N3 Class: N(5.5.6.8.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory IE. content error

ATM Forum Technical Committee B-90

E: SETUP

EQ: non-mandatory error (length of BSC= 6). Note 2,5,21,31. Event: 747

R: NO RESPONSE

NS: N1

Class: N(5.5.6.8.2)

E: SETUP

EQ: non-mandatory error (length of BSC= 6). Note 3,5,21,31. Event: 747

R: CALL PROC

RQ: with a valid CI. NS: N3

Class: N(5.5.6.8.2) E: SETUP

EQ: non-mandatory error (length of BSC= 6). Note 2,5,21,32. Event: 747

R: STATUS RQ: CA/value = 100, CS/state = N1. NS: N1

Class: N(5.5.6.8.2) E: SETUP

EQ: non-mandatory error (length of BSC= 6). Note 3,5,21,32. Event: 747

R: CALL PROC + STATUS RQ: with a valid CI. CA/value = 100, CS/ state = N3. NS: N3 Class: N(5.5.6.8.2) E: SETUP EQ: non-mandatory error (BSC/indication = 1111111B). Note 2,5,21,31. Event: 748

R: NO RESPONSE

NS: N1

Class: N(5.5.6.8.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory IE. content error

B-91 ATM Forum Technical Committee

E: SETUP EQ: non-mandatory error (BSC/indication = 1111111B). Note 3,5,21,31.

Event: 748

R: CALL PROC

RQ: with a valid CI.

NS: N3

Class: N(5.5.6.8.2) E: SETUP EQ: non-mandatory error (BSC/indication = 1111111B). Note 2,5,21,32.

Event: 748

R: STATUS RQ: CA/value = 100, CS/state = N1.

NS: N1

Class: N(5.5.6.8.2)

E: SETUP EQ: non-mandatory error (BSC/indication = 1111111B). Note 3,5,21,32.

Event: 748

R: CALL PROC + STATUS RQ: with a valid CI. CA/value = 100, CS/ state = N3. NS: N3 Class: N(5.5.6.8.2) E: SETUP EQ: non-mandatory error (TNS/type of network = 111B). Note 2,5,11,21,31.

Event: 749

R: NO RESPONSE

NS: N1

Class: N(5.5.6.8.2)

E: SETUP EQ: non-mandatory error (TNS/type of network = 111B). Note 3,5,11,21,31.

Event: 749

R: CALL PROC

RQ: with a valid CI.

NS: N3

Class: N(5.5.6.8.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory IE. content error

ATM Forum Technical Committee B-92

E: SETUP EQ: non-mandatory error (TNS/type of network = 111B). Note 2,5,11,21,32.

Event: 749

R: STATUS RQ: CA/value = 100, CS/state = N1.

NS: N1

Class: N(5.5.6.8.2)

E: SETUP EQ: non-mandatory error (TNS/type of network = 111B). Note 3,5,11,21,32.

Event: 749

R: CALL PROC + STATUS RQ: with a valid CI. CA/value = 100, CS/ state = N3. NS: N3 Class: N(5.5.6.8.2) E: SETUP EQ: non-mandatory error (TNS/network id plan = 1111B). Note 2,5,11,21,31.

Event: 750

R: NO RESPONSE

NS: N1

Class: N(5.5.6.8.2)

E: SETUP EQ: non-mandatory error (TNS/network id plan = 1111B). Note 3,5,11,21,31.

Event: 750

R: CALL PROC

RQ: with a valid CI.

NS: N3

Class: N(5.5.6.8.2) E: SETUP EQ: non-mandatory error (TNS/network id plan = 1111B). Note 2,5,11,21,32.

Event: 750

R: STATUS RQ: CA/value = 100, CS/state = N1.

NS: N1

Class: N(5.5.6.8.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory IE. content error

B-93 ATM Forum Technical Committee

E: SETUP EQ: non-mandatory error (TNS/network id plan = 1111B). Note 3,5,11,21,32. Event: 750

R: CALL PROC + STATUS RQ: with a valid CI. CA/value = 100, CS/ state = N3. NS: N3 Class: N(5.5.6.8.2) E: SETUP

EQ: non-mandatory error (TNS/ident. not recognized). Note 11,21. Event: 751

R: RELEASE COMP

RQ: CA/value = 2. NS: N0

Class: N(annex D) E: SETUP

EQ: non-mandatory error (TNS/ident. not valid). Note 11,21. Event: 752

R: RELEASE COMP

RQ: CA/value = 91. NS: N0

Class: N(annex D) E: SETUP

EQ: non-mandatory error (length of BRI = 6). Note 2,5,21,31. Event: 753

R: NO RESPONSE

NS: N1

Class: N(5.5.6.8.2)

E: SETUP

EQ: non-mandatory error (length of BRI= 6). Note 3,5,21,31. Event: 753

R: CALL PROC

RQ: with a valid CI. NS: N3

Class: N(5.5.6.8.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory IE. content error

ATM Forum Technical Committee B-94

E: SETUP

EQ: non-mandatory error (length of BRI= 6). Note 2,5,21,32.

Event: 753

R: STATUS RQ: CA/value = 100, CS/state = N1.

NS: N1

Class: N(5.5.6.8.2) E: SETUP

EQ: non-mandatory error (length of BRI= 6). Note 3,5,21,32.

Event: 753

R: CALL PROC + STATUS RQ: with a valid CI. CA/value = 100, CS/ state = N3. NS: N3 Class: N(5.5.6.8.2) E: SETUP EQ: non-mandatory error (BRI/indication = 1111B). Note 2,5,21,31.

Event: 754

R: NO RESPONSE

NS: N1

Class: N(5.5.6.8.2)

E: SETUP EQ: non-mandatory error (BRI/indication = 1111B). Note 3,5,21,31.

Event: 754

R: CALL PROC

RQ: with a valid CI.

NS: N3

Class: N(5.5.6.8.2) E: SETUP EQ: non-mandatory error (BRI/indication = 1111B). Note 2,5,21,32.

Event: 754

R: STATUS RQ: CA/value = 100, CS/state = N1.

NS: N1

Class: N(5.5.6.8.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory IE. content error

B-95 ATM Forum Technical Committee

E: SETUP EQ: non-mandatory error (BRI/indication = 1111B). Note 3,5,21,32.

Event: 754

R: CALL PROC + STATUS RQ: with a valid CI. CA/value = 100, CS/ state = N3. NS: N3 Class: N(5.5.6.8.2) E: SETUP EQ: non-mandatory error (BRI/spare = 111B). Note 2,5,21.

Event: 755

R: NO RESPONSE

NS: N1

Class: I(5.4.5.1)

E: SETUP EQ: non-mandatory error (BRI/spare = 111B). Note 3,5,21.

Event: 755

R: CALL PROC

RQ: with a valid CI. NS: N3

Class: I(5.4.5.1) E: RELEASE COMP EQ: non-mandatory invalid content (CA/location = 1111B) Note 31. Event: 756

R: NO RESPONSE stop T308N NS: N0

Class: N(5.5.6.8.2)

E: RELEASE COMP

EQ: non-mandatory invalid content (CA/location = 1111B) Note 32. Event: 756

R: STATUS stop T308N RQ: CA/value =100, CS/state = N0.

NS: N0 Class: N(5.5.6.8.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory IE. content error

ATM Forum Technical Committee B-96

E: RELEASE COMP

EQ: non-mandatory invalid content (CA/ value = 0). Note 31. Event: 757

R: NO RESPONSE stop T308N

NS: N0 Class: N(5.5.6.8.2) E: RELEASE COMP

EQ: non-mandatory invalid content (CA/ value = 0) Note 32. Event: 757

R: STATUS stop T308N RQ: CA/value = 100, CS/state = N0. NS: N0 Class: N(5.5.6.8.2) E: RELEASE COMP

EQ: non-mandatory invalid content (CA/ spare = 111B). Event: 758

R: NO RESPONSE stop T308N

NS: N0 Class: I(5.4.5.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory IE. content error.

B-97 ATM Forum Technical Committee

E: SETUP

EQ: unexpected recognized IE (BHL). Note 2,5.6,21,31. Event: 801

R: NO RESPONSE

NS: N1

Class: N(5.5.6.8.3) E: SETUP

EQ: unexpected recognized IE (BHL). Note 3,5,6,21,31. Event: 801

R: CALL PROC

RQ: with a valid CI.

NS: N3 Class: N(5.5.6.8.3) E: SETUP

EQ: unexpected recognized IE (BHL). Note 2,5,6,21,32. Event: 801

R: STATUS

RQ: CS/state = N1,CA/value = 99. NS: N1

Class: N(5.5.6.8.3) E: SETUP

EQ: unexpected recognized IE (BHL). Note 3,5,6,21,32. Event: 801

R: CALL PROC + STATUS RQ: with a valid CI. CS/state = N3, CA/ value = 99. NS: N3 Class: N(5.5.6.8.3) E: SETUP EQ: unexpected recognized IE ( BRI and 2 BLL). Note 2,5,8,21,31.

Event: 802

R: NO RESPONSE

NS: N1

Class: N(5.5.6.8.3)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory unexpected recognized IE.

ATM Forum Technical Committee B-98

E: SETUP EQ: unexpected recognized IE (BRI and 2 BLL). Note 3,5,8,21,31.

Event: 802

R: CALL PROC

RQ: with a valid CI . NS: N3

Class: N(5.5.6.8.3) E: SETUP EQ: unexpected recognized IE ( BRI and 2 BLL). Note 2,5,8,21,32.

Event: 802

R: STATUS RQ: CS/state = N1, CA/value = 43. NS: N1

Class: N(annex C) E: SETUP EQ: unexpected recognized IE (BRI and 2 BLL). Note 3,5,8,21,32.

Event: 802

R: CALL PROC + STATUS RQ: with a valid CI . CS/state = N3, CA/ value = 43. NS: N3 Class: N(annex C) E: SETUP

EQ: unexpected recognized IE (TNS). Note 2,5,10,21,31. Event: 803

R: NO RESPONSE

NS: N1

Class: N(5.5.6.8.3) E: SETUP

EQ: unexpected recognized IE (TNS). Note 3,5,10,21,31. Event: 803

R: CALL PROC

RQ: with a valid CI . NS: N3

Class: N(5.5.6.8.3)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory unexpected recognized IE.

B-99 ATM Forum Technical Committee

E: SETUP

EQ: unexpected recognized IE (TNS). Note 2,5,10,21,32. Event: 803

R: STATUS

RQ: CA/value = 99, CS/state = N1. NS: N1 Class: N(5.5.6.8.3)

E: SETUP

EQ: unexpected recognized IE (TNS). Note 3,5,10,21,32. Event: 803

R: CALL PROC + STATUS RQ: with a valid CI. CA/value = 99, CS/state = N3. NS: N3 Class: N(5.5.6.8.3) E: SETUP

EQ: unexpected recognized IE (CI). Note 2,5,21,31. Event: 804

R: NO RESPONSE

NS: N1

Class: N(5.5.1.2.1)

E: SETUP

EQ: unexpected recognized IE (CI). Note 3,5,21,31. Event: 804

R: CALL PROC

RQ: with a valid CI.

NS: N3 Class: N(5.5.1.2.1) E: SETUP

EQ: nexpected recognized IE (CI). Note 2,5,21,32. Event: 804

R: STATUS RQ: CA/value = 99, CS/state = N1. NS: N1

Class: N(5.5.1.2.1)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory unexpected recognized IE.

ATM Forum Technical Committee B-100

E: SETUP

EQ: nexpected recognized IE. (CI) Note 3,5,21,32.

Event: 804

R: CALL PROC + STATUS RQ: with a valid CI. CA/value = 99, CS/state = N3. NS: N3 Class: N(5.5.1.2.1) E: remote SETUP

EQ: unexpected recognized IE (BHL). Note 6,21.

Event: 805

R: SETUP start T303N RQ: with a valid CI and without BHL. Note 17,18. NS: N6 Class: N(5.5.6.8.3) E: remote SETUP

EQ: unexpected recognized IE (BRI and 2 BLL). Note 8,21.

Event: 806

R: SETUP start T303N RQ: with a valid CI, 1 BLL and may be BRI. Note 17,18. NS: N6 Class: N(5.5.6.8.3) E: remote SETUP

EQ: unexpected recognized IE (TNS). Note 10,21.

Event: 807

R: SETUP start T303N RQ: with a valid CI and without TNS. Note 17,18. NS: N6 Class: N(5.5.6.8.3) E: remote SETUP

EQ: unexpected recognized IE (CI).Note 21.

Event: 808

R: SETUP start T303N RQ: with a valid CI. Note 17,18.

NS: N6 Class: N(5.5.6.8.3)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix

Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory unexpected recognized IE

B-101 ATM Forum Technical Committee

E: CALL PROC

EQ: unexpected recognized IE (BBC). Note 1,31.

Event: 809

R: NO RESPONSE stop T303N, start T310N

NS: N9

Class: N(5.5.6.8.3) E: CALL PROC

EQ: unexpected recognized IE (BBC). Note 1,32.

Event: 809

R: STATUS stop T303N, start T310N RQ: CA/value = 99, CS/state = N9. NS: U9 Class: N(5.5.6.8.3) E: CONN

EQ: unexpected recognized IE (BLL). without CI. Note 13,14,31.

Event: 810

R: CONN ACK stop T303N

NS: N10

Class: N(5.5.6.8.3) E: CONN

EQ: unexpected recognized IE (BLL). without CI . Note 13,14,32.

Event: 810

R: CONN ACK + STATUS stop T303N RQ: CA/value = 43, CS/state = N10. NS: N10 Class: N(5.5.6.8.3) E: CONN

EQ: unexpected recognized IE (CDN). Note 31. Event: 811

R: CONN ACK stop T303N

NS: N10 Class: N(5.5.6.8.3)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory unexpected recognized IE.

ATM Forum Technical Committee B-102

E: CONN

EQ: unexpected recognized IE (CDN). Note 32. Event: 811

R: CONN ACK + STATUS stop T303N RQ: CA/value = 99, CS/state = N10. NS: N10 Class: N(5.5.6.8.3) E: remote CONN

EQ: unexpected recognized IE (BLL). without CI . Note 2,13,14.

Event: 812

R: CONN RQ: with CI and without BLL.

NS: N10 Class: N(5.5.6.8.3) E: remote CONN

EQ: unexpected recognized IE (BLL). without CI . Note 3,13,14.

Event: 812

R: CONN RQ: with CI and without BLL.

NS: N10 Class: N(5.5.6.8.3) E: CONN ACK

EQ: unexpected recognized IE (QOS). Note 16,31.

Event: 813

R: NO RESPONSE

NS: N10

Class: N(5.5.6.8.3) E: CONN ACK

EQ: unexpected recognized IE (QOS). Note 16,32.

Event: 813

R: STATUS

RQ: CA/value = 99, CS/state = N10.

NS: N10 Class: N(5.5.6.8.3)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory unexpected recognized IE

B-103 ATM Forum Technical Committee

E: RELEASE

EQ: unexpected recognized IE (RI).

Event: 814

R: RELEASE COMP RQ: CA/value = 99.

NS: N0

Class: N(5.5.6.8.3) E: RELEASE COMP

EQ: unexpected recognized IE (CI).

Event: 815

R: NO RESPONSE stop T308N

NS: N0 Class: N(5.5.6.8.3) E: RESTART

EQ: unexpected recognized IE (ATD). Note 31. Event: 816

R: RESTART ACK

NS: N0

Class: N(5.5.6.8.3) E: RESTART

EQ: unexpected recognized IE (ATD). Note 32. Event: 816

R: RESTART ACK + STATUS RQ: CR/global value. CA/value = 99,CS/state = Rest 0. NS: N0 Class: N(5.5.6.8.3) E: RESTART

EQ: unexpected recognized IE (CI). RI/class = all channels. Note 31. Event: 817

R: RESTART ACK

NS: N0

Class: N(5.5.5.2)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory unexpected recognized IE

ATM Forum Technical Committee B-104

E: RESTART

EQ: unexpected recognized IE (CI). RI/class = all channels. Note 32.

Event: 817

R: RESTART ACK + STATUS RQ: CR/global value. CA/value = 99, CS/state = Rest 0. NS: N0 Class: N(5.5.5.2) E: STATUS EQ: unexpected recognized IE (BSC). CS/ state = U10, CA/value = 30. Note 31.

Event: 818

R: NO RESPONSE

NS: N10

Class: N(5.5.6.8.3)

E: STATUS EQ: unexpected recognized IE (BSC). CS/ state = U10, CA/value = 30. Note 32.

Event: 818

R: STATUS start T308N RQ: CA/value = 99, CS/state = N10. NS: N10 Class: N(5.5.6.8.3)

E: STATUS ENQ

EQ: unexpected recognized IE (CA).

Event: 819

R: STATUS

RQ: CA/value =30,99, CS/state = N10. NS: N10

Class: N(5.5.6.8.3)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-Non-Mandatory unexpected recognized IE

B-105 ATM Forum Technical Committee

E: AAL ESTABLISH INDICATION

Event: 851

R: NO RESPONSE

NS: N12 Class: N(5.5.6.9) E: AAL ESTABLISH INDICATION

EQ: Note 2,33.

Event: 852

R: NO RESPONSE

NS: N1 Class: N(5.5.6.9) E: AAL ESTABLISH INDICATION

EQ: Note 2,34.

Event: 852

R: STATUS ENQ start T322N

NS: N1 Class: N(5.5.6.9) E: AAL ESTABLISH INDICATION

EQ: Note 3,33.

Event: 852

R: NO RESPONSE

NS: N3 Class: N(5.5.6.9) E: AAL ESTABLISH INDICATION

EQ: Note 3,34.

Event: 852

R: STATUS ENQ start T322N

NS: N3 Class: N(5.5.6.9)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-AAL Reset

ATM Forum Technical Committee B-106

E: AAL ESTABLISH INDICATION

EQ: Note 33.

Event: 853

R: NO RESPONSE

NS: N6 Class: N(5.5.6.9)

R: NO RESPONSE

NS: N9 Class: N(5.5.6.9) E: AAL ESTABLISH INDICATION

EQ: Note 34.

Event: 853

R: STATUS ENQ start T322N

NS: N6 Class: N(5.5.6.9)

R: STATUS ENQ start T322N

NS: N9 Class: N(5.5.6.9) E: AAL ESTABLISH INDICATION EQ: Event: 854

R: STATUS ENQ start T322N

NS: N10 Class: N(5.5.6.9)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error-AAL Reset

B-107 ATM Forum Technical Committee

E: AAL RELEASE IN- DICATION + AAL ESTABLISH CON- FIRM

EQ: Note 2. Event: 871

R: NO RESPONSE

NS: N0 Class: N(5.5.6.10)

E: AAL RELEASE IN- DICATION + AAL ESTABLISH CON- FIRM

EQ: Note 3. Event: 871

R: NO RESPONSE

NS: N0 Class: N(5.5.6.10)

E: AAL RELEASE IN- DICATION + AAL ESTABLISH CON- FIRM

Event: 872

R: NO RESPONSE

NS: N0 Class: N(5.5.6.10)

R: NO RESPONSE

NS: N0 Class: N(5.5.6.10)

R: NO RESPONSE

NS: N0 Class: N(5.5.6.10)

E: AAL RELEASE IN- DICATION + AAL ESTABLISH CON- FIRM+ (before the expiry of T309N) EQ: Event: 873

R: STATUS ENQ stop T309N start T322N

NS: N10 Class: N(5.5.6.10)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Error AAL Failure

ATM Forum Technical Committee B-108

E: first expiry of T303N.

EQ: Note 35 . Event: 901

R: NO RESPONSE

NS: N0 Class: V(5.5.2.5.4) E: first expiry of T303N.

EQ: Note 36.

Event: 901

R: SETUP restart T303N RQ: Note 17,18.

NS: N6 Class: V(5.5.2.1) E: final expiry of T303N.

EQ: Note 36.

Event: 902

R: NO RESPONSE

NS: N0 Class: V(5.5.2.5.4) E: first expiry of T303N (remote port).

EQ: Note 2,35. Event: 903

R: RELEASE COMP

RQ: CA/value = 18.

NS: N0 Class: V(5.5.2.5.4) E: first expiry of T303N (remote port).

EQ: Note 3,35. Event: 903

R: RELEASE start T308N RQ: CA/value = 18.

NS: N12 Class: V(5.5.2.5.4)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Timers

B-109 ATM Forum Technical Committee

E: final expiry of

T303N (remote port).

EQ: Note 2,36. Event: 904

R: RELEASE COMP

RQ: CA/value = 18.

NS: N0 Class: V(5.5.2.5.4) E: final expiry of

T303N (remote port).

EQ: Note 3,36. Event: 904

R: RELEASE start T308N RQ: CA/value = 18.

NS: N12 Class: V(5.5.2.5.4) E: first expiry of

T308N.

Event: 905

R: RELEASE restart T308N RQ: optionaly 2nd CA/value = 102. NS: N12 Class: V(5.5.4.4) E: final expiry of

T308N.

Event: 906

R: NO RESPONSE stop T308N

NS: N0 Class: V(5.5.4.4) E: AAL RELEASE IN- DICATION + AAL ESTABLISH CON- FIRM (after first expiry of T309N)

Event: 907

R: remote RELEASE start T308N RQ: CA/value = 27.

NS: N0 Class: V(5.5.6.10)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Timers

ATM Forum Technical Committee B-110

E: expiry of T310N.

Event: 908

R: RELEASE start T308N RQ: CA/value = 102.

NS: N12 Class: V(5.5.2.5.4) E: expiry of T310N (remote port).

EQ: Note 2.

Event: 909

R: RELEASE COMP

RQ: CA/value = 18.

NS: N0 Class: V(5.5.2.5.4) E: expiry of T310N (remote port).

EQ: Note 3.

Event: 909

R: RELEASE start T308N RQ: CA/value = 18.

NS: N12 Class: V(5.5.2.5.4) E: AAL ESTABLISH INDICATION + first expiry of T322N. EQ: Event: 910

R: STATUS ENQ restart T322N

NS: N10

Class: V(5.5.6.11)

E: AAL ESTABLISH INDICATION + expiry of T322N (maximum number). EQ: Event: 911

R: RELEASE start T308N RQ: CA/value = 41.

NS: N12 Class: V(5.5.6.11)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

Timers

B-111 ATM Forum Technical Committee

E: STATUS ENQ EQ: Note 2.

Event: 951

R: STATUS RQ: CA/value = 30, CS/state = N1. NS: N1 Class: V(5.5.6.11) E: STATUS ENQ EQ: Note 3.

Event: 951

R: STATUS RQ: CA/value = 30, CS/state = N3. NS: N3 Class: V(5.5.6.11) E: STATUS ENQ

Event: 952

R: STATUS RQ: CA/value = 30, CS/state = N0. NS: N0 Class: V(5.5.6.11)

R: STATUS RQ: CA/value = 30, CS/state = N6. NS: N6 Class: V(5.5.6.11)

R: STATUS RQ: CA/value = 30, CS/state = N9. NS: N9 Class: V(5.5.6.11)

R: STATUS RQ: CA/value = 30, CS/state = N10. NS: N10 Class: V(5.5.6.11)

R: STATUS RQ: CA/value = 30, CS/state = N12. NS: N12 Class: V(5.5.6.11) E: STATUS EQ: CS/state not equal to U0, CA/value = 30.

Event: 953

R: RELEASE COMP RQ: CA/value = 101. NS: N0 Class: I(5.5.6.12 a) E: STATUS EQ: CS/state = U0, CA/value = 30. Note 2.

Event: 954

R: NO RESPONSE

NS: N0 Class: I(5.5.6.12 c)

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

STATUS Enquiry Procedure

ATM Forum Technical Committee B-112

E: STATUS EQ: CS/state = U0, CA/value=30. Note 3.

Event: 954

R: NO RESPONSE

NS: N0 Class: I(5.5.6.12 c) E: STATUS EQ: CS/state = U0. CA/value = 30.

Event: 955

R: NO RESPONSE

NS: N0 Class: V(5.5.6.12 )

R: NO RESPONSE

NS: N0 Class: I(5.5.6.12 c)

R: NO RESPONSE

NS: N0 Class: I(5.5.6.12 c)

R: NO RESPONSE

NS: N0 Class: I(5.5.6.12 c)

R: NO RESPONSE

NS: N0 Class: I(5.5.6.12 c) E: STATUS EQ: CS/state = U10, CA/value = 30. Event: 956

R: NO RESPONSE

NS: N10 Class: V(5.5.6.12 ) E: STATUS EQ: CR/global value..

Event: 957

R: NO RESPONSE

NS: N0 Class: V(5.5.6.12 )

Service Name: ATM UNI 3.1 Signalling Network Side Conformance Test Matrix Specification Reference: UNI 3.1 ATM Forum User Network Interface Specification

State Description

Null Call Initiated Outgoing Call Proceeding

Call Present Incoming Call Proceeding

Active Release Indication

Event SN:^{N0} SN:^{N1} SN:^{N3} SN:^{N6} SN:^{N9} SN:^{N10} SN:^{N12}

STATUS Enquiry Procedure

Notes

ATM Forum Technical Committee B-113

Notes

1: The SETUP is without any optional IE. 2: The Network does not generate a CALL PROCEEDING after receiving a SETUP from the user. 3: The Network generates a CALL PROCEEDING after receiving a SETUP from the user. 4: With all allowable Traffic combination (variation of BBC Class, ATD and QOS Class). 5: With all allowable Traffic combination (Variation of BBC Class ) QOS Class = 0. 6: The Network does not support the BHL. 7: The Network supports the BHL. 8: The Network does not support repetition of the BLL. 9: The Network supports repetition of the BLL. 10: The Network does not support the TNS. 11: The Network supports the TNS. 12: The SETUP is with AALP IE. 13: The SETUP is with BLL IE. 14: The Network does not transport BLL to the calling user. 15: The Network transports BLL to the calling user. 16: The CONNECT ACKNOWLEDGE message is sent in response to a CONNECT message from the Network.

17: The SETUP from the Network to user must contain CGN IE if the Network always includes the calling number in the SETUP message.

18: The SETUP from the Network to user must contain BSC IE if the Network always includes the BSC in the SETUP message.

19: The Network can be configured with all virtual channels busy. 20: The Network does not include the calling number in the SETUP message. 21: With Calling Party Number IE, if the IUT needs this information. 22: The SETUP from the user to the Network contains duplicated mandatory IE. (ATD (2 times), BBC (2 times), CDN(2 times), QOS(2 times)).

23: The SETUP from the user to the Network contains duplicated non-mandatory IE. (AALP (2 times), CGN (2 times)).

24: The SETUP from the user to the Network contains duplicated non-mandatory IE. (BHL (2 times)).

Notes

B-114 ATM Forum Technical Committee

25: The SETUP from the user to the Network contains duplicated non-mandatory IE. (BLL (4 times), BRI(2 times)).

26: The SETUP from the user to the Network contains duplicated non-mandatory IE. (BSC (2 times)). 27: The SETUP from the user to the Network contains duplicated non-mandatory IE. (TNS (2 times)). 28: When a message is received with MT octet 2 flag = 1, the IUT follows the explicit instruction in the Action Indicator.

29: When a message is received with MT octet 2 flag = 1, the IUT shall treat the message as if received with flag = 0.

30: Only if E.164 (Public address) is used. 31: The Nework does not support the sending of STATUS. 32: The Network supports the sending of STATUS. 33: The Network does not support the STATUS ENQUIRY procedure. 34: The Network supports the STATUS ENQUIRY procedure. 35: The Network does not support the retransmission of SETUP. 36: The Network supports the retransmission of SETUP.

Legend

ATM Forum Technical Committee B-115

Legend

AALP ATM Adaptation Layer Parameters. ALERT ALERTING Message. ATD ATM Traffic Descriptor. BBC Broadband Bearer Capability. BHL Broadband High Layer information. BLL Broadband Low Layer information. BLSH Broadband Locking Shift. BNSH Broadband Non-Locking Shift. BRI Broadband Repeat Indicator. BSC Broadband Sending Complete. CA Cause. CALL PROC Call PROCEEDING Message. CONN CONNECT Message. CONN ACK CONNECT ACKNOWLEDGE Message. CDN Called Party Number. CDS Called Party Subaddress. CGN Calling Party Number. CGS Calling Party Subaddress. CI Connection Identifier. CR Call Reference. CS Call State. QOS Quality Of Service parameter. RELEASE COMP RELEASE COMPLETE Message. RESTART ACK RESTART ACKNOWLEDGE Message RI Restart Indicator. MT Message Type. STATUS ENQ STATUS ENQUIRY Message. TNS Transit Network Selection. T303N Timer T303 Network Side. T308N Timer T308 Network Side. T309N Timer T309 Network Side.

Legend

B-116 ATM Forum Technical Committee

T310N Timer T310 Network Side. T322N Timer T322 Network Side. PCR Peak Cell Rate. UNRECOGNIZED Unrecognized Message. > More than.