TABLE 1/T.100

Display modes and control characters-serial mode

Display mode

Set at

Set after

(see Note)

Complementary display mode

Set at

Set after

(see Note)

Alphanumerics

Row start

4/1 4/2 4/3

4/4 4/5 4/6 4/7

Block mosaics

-

5/1 5/2 5/3

5/4 5/5 5/6 5/7

Contiguous

Row start 5/9

5/9

Separated

5/10

5/10

Fore-

ground display colour

includes red

Row start

4/1 4/3 4/5 4/7

5/1 5/3 5/5 5/7

Fore-

ground display colour

includes red

-

4/2 4/4 4/6

5/2 5/4 5/6

includes green

Row start

4/1 4/2 4/3 4/7

5/1 5/2 5/3 5/7

excludes green

-

4/1 4/4 4/5

5/1 5/4 5/5

includes blue

Row start

4/4 4/5 4/6 4/7

5/4 5/5 5/6 5/7

excludes blue

-

4/1 4/2 4/3

5/1 5/2 5/3

Black background

Row start 5/12

-

New background colour

5/13

-

Stop conceal

Row start

4/1 4/2 4/3

4/4 4/5 4/6 4/7

5/1 5/2 5/3

5/4 5/5 5/6 5/7

Conceal

5/8

-

Steady

Row start 4/9

-

Flash

-

4/8

Unboxed

Row start 4/10

4/10

Boxed

4/11

4/11

Normal height

Row start 4/12

-

Double height

-

4/13

Release

Row start

5/15

Hold

5/14

-

Note - All attribute control characters are preceded by Escape ESC.