Recommendation U.44

1)	Replace Point 2, last sentence, by the following:

"This also applies to the RDI condition, in which case the call will not be extended to a redirected subscriber."

2)	Point 3, "Recommendation E.60" should read

"Recommendation F.60".

3)	Point 6, b), "... the calling subscriber commence the..." should read "... the calling subscriber commences the...".

4)	Point 6, c), "... exchange, it if can..." should read

"... exchange, if it can...".

5)	Point 11, replace by the following:

"11.	Clearing of a broadcast call, in response to the clear signal from the originating subscriber, shall comply with the relevant U-Series Recommendations.

For new systems, and as far as possible for existing ones, should the originating subscriber wish to know those parties who cleared prematurely (and, by implication, those who received the complete message) then this should be signalled by terminating the transmitted text with the letter shift MMMM. The originating exchange will then clear forward in the normal way, list those subscribers, if any, who cleared early to the originating subscriber and clear backwards.

Note - Application of this procedure to destinations which use code conversion facilities is a matter for further study."