Technical CommitteeAddendum to UNI Signalling V4.0for ABR parameter negotiationaf-sig-0076.000January, 1997 af-sig-0076.000Addendum to UNI Signalling V4.0 for ABR parameter negotiation2ATM Forum Technical CommitteeAddendum to UNI Signalling V4.0 for ABR parameter negotiationaf-sig-0076.000' 1996 The ATM Forum. All Rights Reserved. No part of this publication may be reproduced in any form or byany means.The information in this publication is believed to be accurate as of its publication date. Such information is subjectto change without notice and The ATM Forum is not responsible for any errors. The ATM Forum does not assumeany responsibility to update or correct any information in this publication.Notwithstanding anything to the contrary, neither The ATM Forum nor the publisher make representation orwarranty, expressed or implied, concerning the completeness, accuracy, or applicability of any information containedin this publication. No liability of any kind shall be assumed by The ATM Forum or the publisher as a result ofreliance upon any information contained in this publication.The receipt or any use of this document or its contents does not in any way create by implication or otherwise:• Any express or implied license or right to or under any ATM Forum member company�s patent, copyright,trademark or trade secret rights which are or may be associated with the ideas, techniques, concepts orexpressions contained herein; nor• Any warranty or representation that any ATM Forum member companies will announce any product(s) and/orservice(s) related thereto, or if such announcements are made, that such announced product(s) and/or service(s)embody any or all of the ideas, technologies, or concepts contained herein; nor• Any form of relationship between any ATM Forum member companies and the recipient or user of thisdocument.Implementation or use of specific ATM standards or recommendations and ATM Forum specifications will bevoluntary, and no company shall agree or be obliged to implement them be virtue of participation in The ATMForum.The ATM Forum is a non-profit international organization accelerating industry cooperation on ATM technology.The ATM Forum does not, expressly or otherwise, endorse or promote any specific products or services.NOTE: The user�s attention is called to the possibility that implementation of the ATM interoperabilityspecification contained herein may require the use of an invention covered by patent rights held by ATM Forummember companies or others. By publication of this ATM interoperability specification, no position is taken by TheATM Forum with respect to validity of any patent claims or of any patent rights related thereto or the ability toobtain the license to use such rights. ATM Forum member companies agree to grant licenses under the relevantpatents they own on reasonable and nondiscriminatory terms and conditions to applicants desiring to obtain such alicense. For additional information contact:The ATM ForumWorldwide Headquarters2570 West El Camino Real, Ste 304Mountain View, CA, CA 94040-1313Tel: +1-415-949-6700Fax: +1-415-949-6705

Addendum to UNI Signalling V4.0 for ABR parameter negotiationaf-sig-0076.000ATM Forum Technical Committee3Section 10.2.1.1 of UNI Signalling V4.0, �QoS and traffic parameter selection procedures�, is modified asfollows.Under �Procedures for parameter defaulting� in the first bullet, change the default value of RIF and add adefault value for RDF:..., for RIF, the default value is 1 which is encoded as 15 (decimal), and for RDF, the default value is 1/32,768which is encoded as 0.In the table later in the same section (�summarizes the modifications that can be made�), replace the linefor RDF as follows:Parameter for agiven directionModification bythe network......RDFNote 1Below the table, delete the existing Note and add the following text:Note 1: The value of RDF may be increased or decreased, subject to the constraint that the ratio RDF / RIF shallnot be decreased. (Hence, if RIF is decreased by a factor k, RDF may be decreased by at most a factor k, or it may beincreased.)